--------------- 22DISK Definitions for foreign disk formats ---------
--------------- they make sense when you're dealing with Europe ------
--------------- All AMSTRAD Definitions and some C128 Definitions ----
--------------- Most of them defined and all tested by H.Jungkunz ----


BEGIN AMS1  Amstrad PCW8256 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS2  Amstrad PCW8256 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS3  Amstrad PCW8256 - SSDD 48 tpi 3" (JOYCE-SYSTEM)
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 07  EXM 0  DSM 174  DRM 63    AL0 0C0H  AL1 0     OFS 1
END

BEGIN AMS4  Amstrad CPC System - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMS5  Amstrad CPC-Data - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 193,194,195,196,197,198,199,200,201
BSH 3  BLM 7  EXM 0  DSM 179  DRM 63    AL0 0C0H  AL1 0     OFS 0
END

BEGIN AMS6  Amstrad B360K - SSDD 96 tpi 5.25"  SKEW 2
DENSITY MFM,LOW
CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 4  BLM 15  EXM 1  DSM 174  DRM 63    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS7  Amstrad VORTEX - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS8  Amstrad CPC System DSDD 96tpi 5.25" - DOBBERTIN -
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS9  Amstrad DOBBERTIN DATA DSDD 96 tpi 5.25" Skew 5
DENSITY MFM,LOW
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201
SIDE2 1 193,194,195,196,197,198,199,200,201
BSH 5  BLM 31  EXM 3  DSM 179  DRM 127   AL0 080H  AL1 0     OFS 0
END

BEGIN AMSA  Amstrad PCW8256 - DSDD 96 tpi 5.25" 10 x 512 788K
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
LABEL AMSA
BSH 5  BLM 31  EXM 3  DSM 197  DRM 255    AL0 0C0H  AL1 0     OFS 1
END

BEGIN AMSB  Amstrad PCW 8512 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 175 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN AMSC  Amstrad PCW 8512 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS5
BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN AMSD  Amstrad PCW 8512 - DSDD 96 tpi 5.25"
SEE AMS1

BEGIN AMSE  Amstrad CPC 6128 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 175 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMSF  Amstrad CPC 6128 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 175 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN AMSG  Amstrad CPC 6128 Side 0 - SSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512
SIDE1 0 193,194,195,196,197,198,199,200,201
BSH 3 BLM 7 EXM 0 DSM 180 DRM 63 AL0 0C0H AL1 0 OFS 0
END 

BEGIN AMSH  Amstrad CPC 6128 Side 1 - SSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 193,194,195,196,197,198,199,200,201
SIDE2 0 193,194,195,196,197,198,199,200,201
BSH 3 BLM 7 EXM 0 DSM 180 DRM 63 AL0 0C0H AL1 0 OFS 80
ORDER EAGLE SKIP
END

BEGIN AMSI  Amstrad CPC464 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3 BLM 7 EXM 0 DSM 171 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMSJ  Amstrad CPC464 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 5 BLM 31 EXM 3 DSM 87 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN AMSK  Amstrad PCW w/DU49 - DSDD 3.5"
DENSITY MFM ,LOW
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 5 BLM 31 EXM 3 DSM 198 DRM 255 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COMA  C128 Juggler MG1581 - DSQD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE2 0 1,2,3,4,5,6,7,8,9,10
SIDE1 1 1,2,3,4,5,6,7,8,9,10
ORDER sides
BSH 4  BLM 15  EXM 0  DSM 390  DRM 127  AL0 0C0H     AL1 0    OFS 4
END

BEGIN COMB  C128 Juggler Maxi 1581 - DSQD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE2 0 1,2,3,4,5
SIDE1 1 1,2,3,4,5
ORDER sides
BSH 4  BLM 15  EXM 0  DSM 400 DRM 127  AL0 0C0H     AL1 0    OFS 0
END

BEGIN COMC  C128 native CP/M DSQD 3.5" Only okay for first half of disk!!!
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE2 0 1,2,3,4,5,6,7,8,9,10
SIDE1 1 1,2,3,4,5,6,7,8,9,10
ORDER sides
BSH 4  BLM 15  EXM 0  DSM 390  DRM 127  AL0 0C0H     AL1 0    OFS 0
END

BEGIN KAY4  Kaypro 2X/4/10 - DSDD 48 tpi 5.25" C128 Version
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER sides
LABEL KAY4
BSH 4  BLM 15  EXM 1  DSM 199  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

------------- Regards ---
------------- Helmut Jungkunz ---
