InS_StArT
NE2100.COM
1.1
^Novell Ethernet NE2100,NE2100.COM,IE0000
?Only one NE2100 can be installed in a machine. It must be in a 16 bit expansion slot.
!RIE0000(INT)Hardware Interrupt
@3
4
5
9
!RIE0000(PORT)Base I/O Port
@300
320
340
360
!RIE0000(DMA)DMA Channel
3
@5
6
7
$OIE0000(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0000(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD

VeRsIoN=2.00  Novell NE2100 Ethernet MLID installation file.
CoPyRiGhT=(c) Copyright 1993 - 1996, by Novell, Inc. All rights reserved.

