InS_StArT
MADGEODI.COM
1.0,MDGDOS29.BIN
^Madge Smart 16 Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 PC Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 PCMCIA Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 AT Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 AT Plus Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client Plus Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client PnP Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 MC Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 MC32 Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 EISA Ringnode,MADGEODI.COM,0E0
^Madge Smart 16/4 PCI Ringnode,MADGEODI.COM,IE0
?This driver requires the download file MDGDOS29.BIN. If your network is using Source Routing please load the ROUTE.COM file after the MADGEODI.COM file.
$OIEM(PORT) Base I/O Port
?Enter the Base I/O Location of the Ringnode to be used. This parameter is not required if there is just a single Madge Smart Ringnode in your machine.
0000
FFFF
$OIEM(SLOT) Bus Slot number
?Enter the Bus slot location of the Ringnode to be used. This parameter is not required if there is just a single Madge Smart Ringnode in your machine.
0
FFFF
!OIEM(FRAME) Frame Type
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIEM(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
!OIEM(MAX FRAME SIZE) Maximum frame size
?Select the maximum packet size for your network. Default is 4210.
626
1138
2162
4210
8200
18000
InS_EnD
