NOTE 	THIS IS THE DATABASE FOR VERSION 1.38 OF 22DISK BY SYDEX.
NOTE 
NOTE 		CONTACT:
NOTE 			SYDEX
NOTE 			P.O. BOX 5700
NOTE 			EUGENE, OR  97405
NOTE 			(503) 683-6033 (voice)
NOTE 			(503) 683-1622 (FAX)

BEGIN A1  Generic CP/M - SSSD 8"
DENSITY FM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABC1  ABC-80 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,8,15,6,13,4,11,2,9,16,7,14,5,12,3,10
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABD1  A. B. Dick Magna III - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 0 17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 255 AL0 0FFH AL1 0 OFS 4
END 

BEGIN ACT1  Actrix (Access Matrix) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ACT2  Actrix (Access Matrix) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 1 1,4,7,2,5,8,3,6,9
SIDE2 1 1,4,7,2,5,8,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ADL1  Adler Textriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN ADV1  Advanced Digital Super 6 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 4,1024
SIDE1 0 1,2,3,4
BSH 4 BLM 15 EXM 0 DSM 77 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN ADV2  Advanced Digital Super 6 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 0 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADV3  Advanced Digital Super 6 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 4,1024 SKEW 2
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 300 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADV4  Advanced Digital Super 8 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 608 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ADV5  Advanced Digital TurboDOS 312K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 0 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADV6  Advanced Digital TurboDOS 366K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 182 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN ADV7  Advanced Controls - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 385 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN ALL1  Allen-Bradley Advisor+ - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 318 DRM 127 AL0 0C0H AL1 0 SOFS 1
END 

BEGIN ALT1  Altos - SSSD 8"
DENSITY FM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,
 20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ALT2  Altos - DSSD 8"
DENSITY FM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
SIDE2 1 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 122 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ALT3  Altos - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 15,512 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
BSH 5 BLM 31 EXM 3 DSM 139 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ALT4  Altos - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 15,512 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 284 DRM 255 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 176 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
LABEL AMI1
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMI2  Amigo - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES LABEL AMI2
BSH 4 BLM 15 EXM 0 DSM 195 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN AMP2  Ampro - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26
SIDE2 1 17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMP4  Ampro - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 17,18,19,20,21
SIDE2 1 17,18,19,20,21
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN AMP5  Ampro - SSDD 3.5"
SEE AMP3

BEGIN AMP6  Ampro - DSDD 3.5"
SEE AMP4

BEGIN AMS1  Amstrad PCW 8256 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN AMS2  Amstrad CPC464 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3 BLM 7 EXM 0 DSM 171 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMS3  Amstrad CPC464 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 5
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 5 BLM 31 EXM 3 DSM 87 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN AMS4  Amstrad PCW 8512 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 175 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN AMS5  Amstrad PCW 8512 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS5
BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN AMS6  Amstrad PCW 8512 - DSDD 96 tpi 5.25"
SEE AMS1

BEGIN AMS7  Amstrad CPC 6128 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 175 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMS8  Amstrad CPC 6128 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 175 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN AMS9  Amstrad CPC 6128 Side 0 - SSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512
SIDE1 0 193,194,195,196,197,198,199,200,201
BSH 3 BLM 7 EXM 0 DSM 180 DRM 63 AL0 0C0H AL1 0 OFS 0
END 

BEGIN AMSA  Amstrad CPC 6128 Side 1 - SSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 193,194,195,196,197,198,199,200,201
SIDE2 0 193,194,195,196,197,198,199,200,201
BSH 3 BLM 7 EXM 0 DSM 180 DRM 63 AL0 0C0H AL1 0 OFS 80
ORDER EAGLE SKIP 
END 

BEGIN AMSB  Amstrad PCW w/DU49 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 198 DRM 255 AL0 0C0H AL1 0 OFS 1
END 

BEGIN ARC1  Archive I - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ARC2  Archive II & III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES EVEN-ODD 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 319 AL0 0F8H AL1 0 OFS 2
END 

BEGIN ARI1  Arisia - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 147 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ASO1  Associate - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 195 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ATR1  ATR-8000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024 SKEW 3
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ATR2  ATR-8000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024 SKEW 3
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN AVA1  Avatar - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BEE1  Beehive - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
SIDE2 1 2,5,8,1,4,7,10,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BEE3  Beehive Microbee - SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BEL1  Computer Bell - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE2 1 0,1,2,3,4,5,6,7,8,9
SIDE1 0 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 192 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BIG1  Big Board (512 bytes/sector) - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 15,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
BSH 4 BLM 15 EXM 0 DSM 280 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BIG2  Big Board (512 bytes/sector) - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 15,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 569 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BIT1  Bitelex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 131 DRM 95 AL0 0E0H AL1 0 OFS 2
END 

BEGIN BMC1  BMC IF800 Model 20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,7,13,19,5,11,17,3,9,15
SIDE2 1 1,7,13,19,5,11,17,3,9,15
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BON3  Bondwell 2 - SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BTI1  BTI Systems - DSDD 48 tpi
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8
SIDE2 1 0,1,2,3,4,5,6,7,8
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 175 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BUR1  Burr-Brown - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256
SIDE1 0 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
SIDE2 1 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN CAL1  Cal-PC - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS1  Cashcom 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 303 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS2  Casio FP-1100/FP-1020 - DSDD 48 tpi 5.25"
SEE FUJ2

BEGIN CCS1  CCS (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
SIDE2 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 165 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS2  CCS (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 0 1,4,7,10,3,6,9,2,5,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS3  CCS (1024 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 0 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS4  CCS 8 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024
SIDE1 0 1,4,7,2,5,8,3,6
SIDE2 1 1,4,7,2,5,8,3,6
ORDER SIDES 
BSH 6 BLM 63 EXM 7 DSM 149 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN CDI1  CDI-5000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN CMC1  CMC Supersystem 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN COI1  Coin - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 392 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN COL1  Coleco ADAM, 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 1,6,3,8,5,2,7,4
BSH 3 BLM 7 EXM 0 DSM 146 DRM 63 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COL2  Coleco ADAM, 254K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,6,3,8,5,2,7,4
SIDE2 0 1,6,3,8,5,2,7,4
ORDER EAGLE 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COL3  Coleco ADAM, 320K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,6,3,8,5,2,7,4
SIDE2 0 1,6,3,8,5,2,7,4
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 152 DRM 63 AL0 080H AL1 0 SOFS 26
END 

BEGIN COL4  Coleco ADAM, 720K - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,5,9,4,8,3,7,2,6
SIDE2 0 1,5,9,4,8,3,7,2,6
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COL5  Coleco ADAM, 360K - DSDD 48 tpi5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
SIDE2 1 1,4,7,2,5,8,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 179 DRM 63 AL0 080H AL1 0 SOFS 4
END 

BEGIN COL6  Coleco ADAM, E&T PROM 720K - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,5,9,4,8,3,7,2,6
SIDE2 1 1,5,9,4,8,3,7,2,6
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COL7  Coleco ADAM, 720K - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,5,9,4,8,3,7,2,6
SIDE2 0 1,5,9,4,8,3,7,2,6
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 358 DRM 127 AL0 0C0H AL1 0 SOFS 4
END 

BEGIN COL8  Columbia Commander 964 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER COLUMBIA 
BSH 4 BLM 15 EXM 1 DSM 190 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN COL9  Columbia 1600 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER COLUMBIA 
BSH 5 BLM 31 EXM 3 DSM 197 DRM 255 AL0 0C0H AL1 0 OFS 2
END 

BEGIN COM1  Compis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 317 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM2  Compugraphic MCS-5 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM3  Compustar Model 30 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 35 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN COM4  Compustar 30, Super IOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 35 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 127 AL0 0c0H AL1 0 OFS 2
END 

BEGIN COM7  Compupro (Viasyn) (1024 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN COM8  Compupro (Viasyn) 8/16 - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 8,1024
SIDE1 0 1,4,7,2,5,8,3,6
BSH 4 BLM 15 EXM 0 DSM 299 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN COM9  Compupro (Viasyn) 8/16 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024
SIDE1 0 1,4,7,2,5,8,3,6
SIDE2 1 1,4,7,2,5,8,3,6
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 599 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN COMA  Commodore 1581 drive  - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE2 0 1,2,3,4,5,6,7,8,9,10
SIDE1 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 397 DRM 127 AL0 0C0H AL1 0 OFS 0
END 

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,128 SKIP 
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN CRO2  Cromemco CDOS - DSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,128 SKIP 
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
SIDE2 1 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 172 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKIP 
SIDE1 0 1,5,9,3,7,2,6,10,4,8
LABEL CRO3
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CRO4  Cromemco CDOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKIP 
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER SIDES LABEL CRO4
BSH 4 BLM 15 EXM 0 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CRO5  Cromemco CDOS - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 16,512 SKIP 
SIDE1 0 1,12,7,2,13,8,3,14,9,4,15,10,5,16,11,6
SIDE2 1 1,12,7,2,13,8,3,14,9,4,15,10,5,16,11,6
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 608 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKIP 
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CRO7  Cromemco CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKIP 
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 1 1,4,7,10,3,6,9,2,5,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CWP1  C/WP Cortex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CYK1  Cykey - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 94 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 195 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
 SEE DEC1

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DIC1  Dictaphone 6000 CP/M - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
SIDE2 1 1,3,5,7,9,2,4,6,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 352 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIG1  Digilog 2500 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 166 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN DIG2  Digilog 1500 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 392 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIR1  Direct 1025 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 152 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIR2  Direct 1025 - DSDD 96 tpi 5.25"
SEE MAI1

BEGIN DIS1  Discovery - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 313 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DUE1  Duet CP/M - DSDD 96tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
SIDE2 1 1,3,5,7,9,2,4,6,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 355 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN EAG1  Eagle II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN EAG2  Eagle III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN ELE1  Electroglas/Xynetics - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512 SKEW 3
SIDE1 240 1,2,3,4,5,6,7,8
SIDE2 242 1,2,3,4,5,6,7,8
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 158 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN ELE2  Electroglas/Xynetics - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 240 1,2,3,4,5,6,7,8,9,10
SIDE2 242 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 397 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN EPS3  Epson PX-10/8 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN EPS4  Epson QX-16 640K - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 304 DRM 127 AL0 0C0H AL1 0 OFS 8
END 

BEGIN EPS5  Epson QX-16 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0FCH AL1 0 OFS 4
END 

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5 BLM 31 EXM 3 DSM 77 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 174 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN ESP1  Esprit DBS 16 - DSDD 96 tpi 5.25"
SEE COI1

BEGIN EUR1  Eureka A4 - DSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
SIDE2 1 2,5,8,1,4,7,10,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 399 DRM 255 AL0 0F0H AL1 0 OFS 0
END 

BEGIN EXI1  Exidy Sorcerer - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SECTORS 16,256 SIDES 1
SIDE1 0 1,6,11,16,5,10,15,4,9,14,3,8,13,2,7,12
BSH 4 BLM 15 EXM 0 DSM 76 DRM 63 AL0 0C0H AL1 0 SOFS 33
END 

BEGIN EXO1  EXO - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 16,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5 BLM 31 EXM 3 DSM 149 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN EXO2  EXO - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 15,512 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 303 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN FG1  F & G Cable Tester - DSDD 3.5"
SEE MIC7

BEGIN FLO1  Florida Graphics - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256 SKEW 2
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 295 DRM 127 AL0 0C0H AL1 0 OFS 12
END 

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
SEE IBM2

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN FUT1  Future FX-20 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 4 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 95 AL0 080H AL1 0 OFS 2
END 

BEGIN GEM1  Gemini Galaxy - 5.25" DSDD 96 tpi
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER EAGLE 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN GNA1  Gnat System 10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN GRA1  Graco OM-5000 - DSHD 5.25"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,
 17,18,19,20,21,22,23,24,25,26
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,
 17,18,19,20,21,22,23,24,25,26
ORDER SIDES SKIP 
BSH 5 BLM 31 EXM 3 DSM 248 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN HAG1  Hagiwara HPU 801 CP/M 68K - DSDD 3.5" Special
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 486 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN HAZ1  Hazeltine - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 77 SIDES 2 SECTORS 10,512 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 379 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN HCL1  HCL System 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 388 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 1 DSM 82 DRM 95 AL0 0C0H AL1 0 OFS 3
END 

BEGIN HEA2  Heath H89, Magnolia CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 95 AL0 0C0H AL1 0 OFS 3
END 

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 3
END 

BEGIN HEU1  Heurikon MLZ-91A - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HEW1  Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 251 DRM 127 AL0 0F0H AL1 0 OFS 3
END 

BEGIN HEW2  Hewlett Packard HP 125 - SSSD 8"
DENSITY FM ,HIGH 
CYLINDERS 66 SIDES 1 SECTORS 16,256 SKEW 6
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
BSH 3 BLM 7 EXM 0 DSM 251 DRM 127 AL0 0F0H AL1 0 OFS 3
END 

BEGIN HEW3  Hewlett Packard HP 125 - SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 66 SIDES 1 SECTORS 16,256 SKEW 6
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
BSH 3 BLM 7 EXM 0 DSM 251 DRM 127 AL0 0F0H AL1 0 OFS 3
END 

BEGIN HIT1  Hitachi HPC-6000 CP/M 68K - DSHD 1.2M 3.5"
SEE NEC3

BEGIN HIT2  Hitachi R-1500 CP/M 68K - DSHD 1.2M 5.25"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 494 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HOU1  Strippit Houdaille Fab/V - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 174 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS LABEL IBM2
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN ICL1  ICL DRS 20 - DSDD 5.25" 96 tpi
DENSITY MFM ,LOW CYLINDERS 80
SIDES 2 SECTORS 16,256 ORDER SIDES 
SIDE1 0 1,6,11,16,5,10,15,4,9,14,3,8,13,2,7,12
SIDE2 1 1,6,11,16,5,10,15,4,9,14,3,8,13,2,7,12
BSH 5 BLM 31 EXM 3 DSM 158 DRM 255 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ICL2  ICL DRS 300 - DSDD 5.25" 96 tpi
DENSITY MFM ,LOW CYLINDERS 80
SIDES 2 SECTORS 9,512 ORDER SIDES 
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 0 DSM 350 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN ICL3  ICL Model 35/36 - DSDD 5.25" 96 tpi
DENSITY MFM ,LOW CYLINDERS 80
SIDES 2 SECTORS 10,512 ORDER SIDES 
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 0 DSM 391 DRM 127 AL0 0C0H AL1 0 SOFS 36
END 

BEGIN IMS1  IMS 5000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,9,2,10,3,11,4,12,5,13,6,14,7,15,8,16
LABEL IMS1
BSH 3 BLM 7 EXM 0 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN IMS2  IMS 5000 TurboDOS - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 390 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN IMS3  IMS 5000 TurboDOS - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
BSH 4 BLM 15 EXM 0 DSM 308 DRM 191 AL0 0E0H AL1 0 OFS 0
END 

BEGIN IMS4  IMS 5000 CP/M - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN INT1  Intel iPDS 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 307 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN INT2  Intuit - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
BSH 3 BLM 7 EXM 0 DSM 190 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN INS1  Insight Enterprises - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ITH1  Ithaca Intersystems - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ITH2  Ithaca Intersystems - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 15,512
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12
BSH 4 BLM 15 EXM 0 DSM 284 DRM 191 AL0 0E0H AL1 0 OFS 1
END 

BEGIN ITH3  Ithaca Intersystems - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 15,512
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 284 DRM 255 AL0 0C0H AL1 0 OFS 1
END 

BEGIN ITT1  ITT 3030 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 3 BLM 7 EXM 0 DSM 247 DRM 63 AL0 0C0H AL1 0 OFS 4
END 

BEGIN ITT2  ITT 3030 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 70 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 270 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN JCI1  JC Information Systems TurboDOS - DSDD 96tpi 5.25"
SEE HCL1

BEGIN JET1  Jet-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN JET2  Jet-80 - DSDD 96 tpi 5.25"
SEE WAV2

BEGIN JON1  Jonos - SSDD 3.5"
DENSITY MFM ,LOW CYLINDERS 70 SECTORS 9,512 SIDES 1
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 1 DSM 152 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 194 DRM 63 AL0 0F0H AL1 0 OFS 1
END 

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 196 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 95 AL0 080H AL1 0 OFS 2
END 

BEGIN KAY4  Kaypro Advent TurboROM - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5
SIDE2 1 11,12,13,14,15
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 195 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN KON1  Kontron - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,4,7,10,13,16,19,22,25,3,6,9,12,15,18,21,24,2,5,8,11,14,17,20,23,26
SIDE2 1 1,4,7,10,13,16,19,22,25,3,6,9,12,15,18,21,24,2,5,8,11,14,17,20,23,26
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 489 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN KON2  Kontron/Zeiss - DSDD 96 tpi 5.25"
DENSITY FM ,LOW CYLINDERS 35 SIDES 2 SECTORS 16,128
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER CYLINDERS 
BSH 3 BLM 7 EXM 0 DSM 106 DRM 63 AL0 0C0H AL1 0 OFS 17
END 

BEGIN KON3  Kontron Transient Recorder- DSDD 96 tpi 5.25" & 3.5"
DENSITY MFM ,LOW CYLINDERS 77 SIDES 2 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 299 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN LAN1  Lanier LTD READ-ONLY - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES SKEW 3
BSH 4 BLM 15 EXM 0 DSM 318 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 77 SIDES 2 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 299 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN LEX1  Lexoriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN LOB1  Lobo Max-80 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 165 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB2  Lobo Max-80 (256) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB3  Lobo Max-80 (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB4  Lobo Max-80 (512 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN LNW1  LNW 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 4 BLM 15 EXM 1 DSM 82 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MAC1  Macsym 150 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MAG1  Magic - DSDD 48 tpi 5.25"
SEE AMI2

BEGIN MAI1  MAI Basic Four - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 312 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN MAR1  Marconi Midata 510 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER EAGLE 
BSH 5 BLM 31 EXM 3 DSM 197 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN MC1  MC CP/M  DSDD 96 tpi 5.25"/3.5"
SEE HCL1

BEGIN MIC1  Micromint SB180 - DSDD 96 tpi 5.25"
SEE AMP4

BEGIN MIC2  Micromint SB180 - DSDD 48 tpi 5.25"
SEE AMP2

BEGIN MIC3  MicroMint SB180 Native 3 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2
SECTORS 10,512
SIDE1 0 27,28,29,30,31,32,33,34,35,36
SIDE2 1 27,28,29,30,31,32,33,34,35,36
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 200 DRM 127 AL0 0C0H AL1 0 OFS 0
END 

BEGIN MIC5  Micron Quark - DSDD 48 tpi 5.25"
SEE MOR6

BEGIN MIC6  Micro Source M6000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 0 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MIC7  Michels and Kleberhoff CP/M 3 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER EAGLE COMPLEMENT 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MIC8  Michels and Kleberhoff CP/M 3 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 35 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN MOL1  Molecular Series 9 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 179 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MOL2  Molecular/Durango Poppy 54 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 128,129,130,131,132,133,134,135,136,137
SIDE2 1 138,139,140,141,142,143,144,145,146,147
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MON1  Monroe 8800 Series - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024
SIDE1 0 1,4,2,5,3
LABEL MOR1
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES 
LABEL MOR2
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN MOR3  Morrow 8 (512 bytes/sector) - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 15,512
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12
BSH 4 BLM 15 EXM 0 DSM 280 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MOR4  Morrow 8 (1024 bytes/sector) - SSDD 8"
SEE COM8

BEGIN MOR5  Morrow 8 (1024 bytes/sector) - DSDD 8"
SEE COM9

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MOS1  MOS 80 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,
 15,24,7,16,25,8,17,26,9,18
SIDE2 1 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,
 15,24,7,16,25,8,17,26,9,18
ORDER SIDES 
BSH 5 BLM 31 EXM 0 DSM 244 DRM 251 AL0 0C0H AL1 0 OFS 3
END 

BEGIN MSD1  MSD Systems PSC-1 POS - DSDD 5.25" 96 tpi
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512 ORDER CYLINDERS 
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
BSH 5 BLM 31 EXM 3 DSM 158 DRM 127 AL0 080H AL1 0 OFS 1
END 

BEGIN NCH1  NCHQ System II - SSSD 48tpi 5.25
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,128
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 3 BLM 7 EXM 0 DSM 84 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER EAGLE LABEL NCR1
BSH 4 BLM 15 EXM 1 DSM 153 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN NCR2  NCR FirstStep - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 276 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN NDR1  NDR - DSDD 96 tpi 5.25"/3.5"
SEE HCL1

BEGIN NEC1  NEC PC-8001A - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN NEC2  NEC PC-8801A - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NEC3  NEC PC-8801A - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 242 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN NEC4  NEC PC 8801A/8831A - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NEC5  NEC PC 8500/8431A, Starlet - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NEC6  NEC Bungo - DSDD 3.5"
SEE SEI1

BEGIN NEC7  NEC PC-8001B - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN NEW1  New Brain - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 1 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 5 BLM 31 EXM 3 DSM 97 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN NIA1  Niat - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN NUM1  Numeridex 7000 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,
 20,26,6,12,18,24,4,10,16,22
SIDE2 1 28,34,40,46,52,32,38,44,50,30,36,42,48,
 27,33,39,45,51,31,37,43,49,29,35,41,47
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 248 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN OCT1  Octagon 8/16 - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 9,1024 SKEW 3
SIDE1 0 0,1,2,3,4,5,6,7,8
BSH 5 BLM 31 EXM 1 DSM 167 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN OKI1  OKI IF800 Model 20 - DSDD 48 tpi 5.25"
SEE BMC1

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
SKIP 
END 

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OLI3  Olivetti 250 -  SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN OLI4  Olivetti CWP1 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 17,19,21,23,25,27,29,31,18,20,22,24,26,28,30,32
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 148 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN OLY3  Olympia Olytext 20 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 312 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OLY4  Olympia People - DSDD 96tpi 5.25"
SEE OLY3

BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 45 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 184 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
 SEE OSB2

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB9  Osborne Executive w/Z3 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 127 AL0 0F8H AL1 0 OFS 2
END 

BEGIN OSBA  Osborne Executive Dig. Arts - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0F8H AL1 0 OFS 2
END 

BEGIN OSBB  Osborne Nuevo 2.1 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 311 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OTR1  Otrona Attache - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 181 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OTR2  Otrona Attache - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 386 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN PEG1  Pegasus Data Logger - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
SIDE2 1 1,4,7,2,5,8,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 80H AL1 0 OFS 6
END 

BEGIN PEO1  People's World Computer - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SKEW 2 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 398 DRM 127 AL0 078H AL1 0 OFS 0
END 

BEGIN PEO2  People's World Computer Boot Disk - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SKEW 2
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 397 DRM 127 AL0 0FH AL1 0 SOFS 0
END 

BEGIN PER1  Pericom - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 0 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PHI2  Philips PC-2012 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4 BLM 15 EXM 1 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN PHY1  Physical Acoutstics - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 3
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 173 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PRI1  Prince Digico - DSDD 96 tpi 5.25"
SEE OSBB

BEGIN PRO1  Proglas 770K - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 388 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN QDP1  QDP-500 - DSHD 5.25" 96 tpi
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024
SIDE1 0 1,3,5,7,2,4,6,8
SIDE2 1 1,3,5,7,2,4,6,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DRM 127 DSM 624 AL0 0F0H AL1 0 OFS 2
END 

BEGIN REM1  Remanco "Back of the House" - DSDD 96 tpi 5.25"
SEE IMS2

BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 155 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN SAN3  Sanyo MBC-2000 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 16,256
SIDE1 0 1,6,11,16,5,10,15,4,9,14,3,8,13,2,7,12
BSH 4 BLM 15 EXM 1 DSM 152 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN SAN4  Sanco 8001 - 5.25" DSDD 48 tpi
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES SKIP 
BSH 4 BLM 15 EXM 0 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SEE1  Seequa Chameleon - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN SEE2  Seequa Chameleon - DSDD 48 tpi 5.25"
SEE IBM2

BEGIN SEI1  Seiko - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES COMPLEMENT 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SHA2  Sharp MZ-80B - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE2 0 1,2,3,4,5,6,7,8,9,10
SIDE1 1 11,12,13,14,15,16,17,18,19,20
ORDER SIDES COMPLEMENT 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SHA3  Sharp 3500/5500 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN SHL1  Shelton SIG/NET 2 - SSDD 48 tpi 5.25"
SEE SUP2

BEGIN SHL2  Shelton SIG/NET 2 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES COMPLEMENT 
BSH 4 BLM 15 EXM 1 DSM 195 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SHL3  Shelton SIG/NET 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES COMPLEMENT 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN SIE1  Siemens PG-685 DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL SIE1
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL SIE2
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN SIE3  Siemens PG-635 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL SIE3
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SIE4  Siemens PG-3101A - DSDD 5.25" 48 tpi
SEE WAN1

BEGIN SMA1  Smart Aleck - SSDD 5.25" 48 tpi
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SOR1  Sorbus TurboDOS - 5.25" DSHD (or 8" DSDD)
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 308 DRM 255 AL0 0C0H AL1 0 OFS 0
END 

BEGIN SON1  Sony SMC-70 - SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 70 SIDES 1 SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4 BLM 15 EXM 1 DSM 135 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 17,256 SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN SPE2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 383 AL0 0FCH AL1 0 OFS 2
END 

BEGIN SPE3  Spectravideo - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 17,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 157 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN SPE4  Spectravideo - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 17,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 163 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN SPE5  Spectravideo - DSDD 48 tpi 5.25"
DENSITY MFM , LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 197 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN SPE6  Spectravideo - SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 1 DSM 163 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 35 SIDES 1 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 81 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 40 SIDES 1 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 35 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP4  Superbrain II - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW COMPLEMENT 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 127 AL0 080H AL1 0 OFS 3
END 

BEGIN SYS1  System Group 2800 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 303 DRM 255 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SYS2  Systel 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN SYS3  Systel 3 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TAR1  Tarbell - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 15,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,12,13,14
SIDE2 0 1,2,3,4,5,6,7,8,9,10,11,12,12,13,14
ORDER SIDES 
BSH 5 BLM 31 EXM 0 DSM 303 DRM 169 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TAT1  Tatung TPC2000 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 3
SIDE1 0 0,1,2,3,4,5,6,7,8
SIDE2 0 0,1,2,3,4,5,6,7,8
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TEC1  Techron TEF 10 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 1 1,4,7,10,3,6,9,2,5,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 319 AL0 0F8H AL1 0 OFS 2
END 

BEGIN TEC2  Techron TEF 12 - DSHD 96 tpi 5.25"
DENSITY MFM ,HIGH CYLINDERS 80 SIDES 2 SECTORS 17,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 670 DRM 767 AL0 0FFH AL1 0F0H OFS 4
END 

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 153 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN TEL1  Teletek - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,256
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,
 20,26,6,12,18,24,4,10,16,22
BSH 4 BLM 15 EXM 1 DSM 242 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TEL2  Teletek Systemaster - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256
SIDE1 0 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
SIDE2 1 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TEL3  Televideo 801, 806 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 6
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TEL5  Televideo 806 TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SKEW 2 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 200 DRM 127 AL0 0C0H AL1 0 OFS 0
END 

BEGIN TEL6  Telcom 6.2 CP/M - DSDD 3.5"
SEE OLY3

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TIK1  TIKI-100, 200K - SSDD 48 tpi 5.25"
SEE AMI1

BEGIN TIK2  TIKI-100, 400K - DSDD 48 tpi 5.25"
SEE AMI2

BEGIN TOK1  Tokyo Electron 80W - 3.5" DSHD
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 6 BLM 63 EXM 3 DSM 160 DRM 255 AL0 080H AL1 0 OFS 0
END 

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 6
END 

BEGIN TOS2  Toshiba 300 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 318 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 0 SIDES 1 SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3 BLM 7 EXM 0 DSM 71 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TRS2  TRS-80 Model 1, Bigmem CP/M - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,256
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,
 20,26,6,12,18,24,4,10,16,22
BSH 4 BLM 15 EXM 1 DSM 243 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS4  TRS-80 Lifeboat CP/M (256 bytes/sector) - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,256
SIDE1 0 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,
 15,24,7,16,25,8,17,26,9,18
BSH 4 BLM 15 EXM 0 DSM 242 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS5  TRS-80, Lifeboat CP/M (1024 bytes/sector) - SSDD 8"
SEE COM8

BEGIN TRS6  TRS-80, Pickles & Trout CP/M - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 16,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 4 BLM 15 EXM 0 DSM 299 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 190 DRM 63 AL0 0F0H AL1 0 OFS 2
END 

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512 SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TRSC  TRS-80 Model 3 - Hurricane CP/M - SSDD 48 tpi 5.25"
SEE MOR1

BEGIN TRSD  TRS-80 Model 4P - Montezuma 800K - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 399 DRM 127 AL0 0C0H AL1 0 OFS 0
END 

BEGIN UMI1  U-Micro 1000 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN VAR1  Varian Spectra AA/20  - 5.25" DSDD
DENSITY MFM ,LOW 
CYLINDERS 40 SECTORS 9,512 SIDES 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 317 DRM 63 AL0 060H AL1 0 SOFS 2
ORDER EAGLE 
END 

BEGIN VEC1  Vector 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 356 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN VIS1  Visual 1050 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 1 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAN1  Wangwriter - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAV2  Wave Mate Bullet - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 31 AL0 080H AL1 0 OFS 3
END 

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 17,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 156 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 17,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
LABEL XER4
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER5  Xerox 16/8 - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,256 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,
 17,18,19,20,21,22,23,24,25,26
BSH 4 BLM 15 EXM 1 DSM 242 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN XER6  Xerox 16/8 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256 SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,
 17,18,19,20,21,22,23,24,25,26
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,
 17,18,19,20,21,22,23,24,25,26
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 246 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN XER7  XEROX 16/8, EM-II  (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN XER8  Xerox 820, S/W Publishers DD - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 3 SKIP 
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 166 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER9  Xerox 3700 Laser Printer - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 17,256 SKEW 3
SIDE1 240 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 242 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XERA  Xerox 1800 - DSDD 96 tpi 3.5"/5.25"
SEE IBM1

BEGIN XOR1  Xor 5 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,6,2,7,3,8,4,9,5,10
SIDE2 0 1,6,2,7,3,8,4,9,5,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XYZ1  XYZ - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN ZEI1  Zeiss Video Analysis System - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 299 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 10,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 91 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES LABEL ZEN2
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES LABEL ZEN3
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES LABEL ZEN4
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
LABEL ZEN5
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES LABEL ZEN6
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL ZEN7
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES LABEL ZEN8
BSH 4 BLM 15 EXM 1 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN9  Zenith Z-100 - SSSD 8"
DENSITY FM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,
 20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ZENA  Zenith Z-100 - SSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 1 SECTORS 26,256
SIDE1 0 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,
 15,24,7,16,25,8,17,26,9,18
BSH 4 BLM 15 EXM 1 DSM 242 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ZENB  Zenith Z-37 Disk - DSDD 96 (Half drive) 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 16,256 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES LABEL ZENB
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZENC  Zenith/Heath H-89 Extended Density - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 195 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEND  Zenith Z-100, Heath H-47 Extended Density - DSDD 8"
SEE ADV4

BEGIN ZENE  Zenith Z-100, Heath H-47 - DSDD 8"
DENSITY MFM ,HIGH 
CYLINDERS 77 SIDES 2 SECTORS 26,256
SIDE1 0 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,15,24,7,16,25,8,17,26,9,18
SIDE2 1 1,10,19,2,11,20,3,12,21,4,13,22,5,14,23,6,15,24,7,16,25,8,17,26,9,18
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 497 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZENF  Zenith Z-37 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 1 SECTORS 5,1024 SKEW 3
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 190 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZENG  Zenith Z-37 ED - DSDD 96 tpi 5.25"
SEE OSBB

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 2
END 

NOTE    THIS IS THE DATABASE FOR VERSION 1.40 OF 22DISK BY SYDEX.
NOTE 
NOTE 			SYDEX
NOTE 			P.O. Box 5700
NOTE 			Eugene, OR  97405
NOTE 			(503) 683-6033

BEGIN A1  Generic CP/M - SSSD 8"
DENSITY FM ,HIGH CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABC1  ABC-80 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,8,15,6,13,4,11,2,9,16,7,14,5,12,3,10
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABD1  A. B. Dick Magna III - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 0 17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 255 AL0 0FFH AL1 0 OFS 4
END 

BEGIN ACT1  Actrix (Access Matrix) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADL1  Adler Textriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN ADV1  Advanced Digital Super 6 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 4,1024
SIDE1 0 1,2,3,4
BSH 4 BLM 15 EXM 0 DSM 77 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN ADV3  Advanced Digital Super 6 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 4,1024
SKEW 2
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 300 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADV5  Advanced Digital TurboDOS 312K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 0 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 176 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMS1  Amstrad PCW8256 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN AMSD  Amstrad PCW 9256, 9512 Disckit - DSDD 3.5"
SEE AMS1

BEGIN ARC1  Archive I - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ARC2  Archive II & III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES EVEN-ODD 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 319 AL0 0F8H AL1 0 OFS 2
END 

BEGIN ARI1  Arisia - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 147 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ATR1  ATR-8000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SKEW 3
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AVA1  Avatar - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BEE1  Beehive - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
SIDE2 1 2,5,8,1,4,7,10,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BIT1  Bitelex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 131 DRM 95 AL0 0E0H AL1 0 OFS 2
END 

BEGIN BMC1  BMC IF800 Model 20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,7,13,19,5,11,17,3,9,15
SIDE2 1 1,7,13,19,5,11,17,3,9,15
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BUR1  Burr-Brown - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
SIDE2 1 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN CAL1  Cal-PC - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS1  Cashcom 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 303 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS2  Casio FP-1100/FP-1020 - DSDD 48tpi 5.25"
SEE FUJ2

BEGIN CCS1  CCS (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
SIDE2 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 165 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS2  CCS (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 0 1,4,7,10,3,6,9,2,5,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS3  CCS (1024 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 0 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CDI1  CDI-5000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN CMC1  CMC Supersystem 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN COL1  Coleco ADAM, 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,6,3,8,5,2,7,4
BSH 3 BLM 7 EXM 0 DSM 146 DRM 63 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COM1  Compis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 317 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM2  Compugraphic MCS-5 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM3  Compustar Model 30 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN COM4  Compupro (Viasyn) (1024 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,128 SKIP 
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512 SKIP 
SIDE1 0 1,5,9,3,7,2,6,10,4,8
LABEL CRO3
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512 SKIP 
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CWP1  C/WP Cortex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CYK1  Cykey - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 94 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
SEE DEC1

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DIG1  Digilog - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 166 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN DIG2  Digilog 1500 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 392 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIR1  Direct 1025 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 152 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIS1  Discovery - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 313 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN EAG1  Eagle II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN EAG2  Eagle III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN EPS3  Epson PX-8 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5 BLM 31 EXM 3 DSM 77 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 174 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN FLO1  Florida Graphics - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 295 DRM 127 AL0 0C0H AL1 0 OFS 12
END 

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
SEE IBM2

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN GNA1  Gnat System 10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HCL1  HCL System 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 1 DSM 82 DRM 95 AL0 0C0H AL1 0 OFS 3
END 

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 3
END 

BEGIN HEU1  Heurikon MLZ-91A - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HP1  Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 251 DRM 127 AL0 0F0H AL1 0 OFS 3
END 

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
LABEL IBM2
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN IMS1  IMS 5000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,9,2,10,3,11,4,12,5,13,6,14,7,15,8,16
BSH 3 BLM 7 EXM 0 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN IMS2  IMS 5000 TurboDOS - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 380 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN INT1  Intel iPDS 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 307 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN INS1  Insight Enterprises - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ITH1  Ithaca Intersystems - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN JET1  Jet-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 194 DRM 63 AL0 0F0H AL1 0 OFS 1
END 

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 196 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 95 AL0 080H AL1 0 OFS 2
END 

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 77
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 299 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN LEX1  Lexoriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN LOB1  Lobo Max-80 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 165 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB3  Lobo Max-80 (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB4  Lobo Max-80 (512 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN LNW1  LNW 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 4 BLM 15 EXM 1 DSM 82 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MAC1  Macsym 150 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MAG1  Magic - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN MAI1  MAI Basic Four - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 312 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN MIC2  Micromint SB180 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26
SIDE2 1 17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MIC3  Micron Quark - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MIC5  Micro Source M6000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 0 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MOL1  Molecular Series 9 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 179 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MOL2  Molecular/Durango Poppy 54 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 128,129,130,131,132,133,134,135,136,137
SIDE2 1 138,139,140,141,142,143,144,145,146,147
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MON1  Monroe 8800 Series - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES LABEL MOR2
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 153 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN NCR2  NCR FirstStep - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 276 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN NEC1  NEC PC-8001A - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN NEC3  NEC PC 8801A/8831A - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 152 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NEC4  NEC PC 8500/8431A, Starlet - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NIA1  Niat - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN OKI1  OKI IF800 Model 20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,7,13,19,5,11,17,3,9,15
SIDE2 1 1,7,13,19,5,11,17,3,9,15
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14, 16,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OLI3  Olivetti 250 -  SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 45 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 184 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 184 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB9  Osborne Executive w/Z3 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 127 AL0 0F8H AL1 0 OFS 2
END 

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 311 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OTR1  Otrona Attache - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 181 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OTR2  Otrona Attache - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 386 DRM 127 AL0 0C0H AL1 00H OFS 3
END 

BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN PEG1  Pegasus Data Logger - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
SIDE2 1 1,4,7,2,5,8,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 80H AL1 0 OFS 6
END 

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4 BLM 15 EXM 1 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PRO2  Proglas 770KB - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 388 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 155 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN SEE1  Seequa Chameleon - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN SEI1  Seiko - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SHL1  Shelton SIG/NET 2 - SSDD 48 tpi 5.25"
SEE SUP2

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SIE1  Siemens  PG-685 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN SIE3  Siemens PG-635 DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SOR1  Sorbus TurboDOS - 5.25" DSHD (or 8" DSDD)
DENSITY MFM ,HIGH 
CYLINDERS 77
SIDES 2
SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 308 DRM 255 AL0 0C0H AL1 0 OFS 0
END 

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN SPE2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 383 AL0 0FCH AL1 0 OFS 2
END 

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 81 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SYS2  Systel 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN SYS3  Systel 3 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 153 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN TEL2  Teletek Systemaster - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
SIDE2 1 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TEL3  Televideo 801, 806 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SKEW 6
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 6
END 

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 0
SIDES 1
SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3 BLM 7 EXM 0 DSM 71 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 190 DRM 63 AL0 0F0H AL1 0 OFS 2
END 

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TRSC  TRS-80 Model 3, Hurricane CP/M - SSDD 48 tpi 5.25"
SEE MOR1

BEGIN VEC1  Vector 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 356 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN VIS1  Visual 1050 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAN1  Wangwriter - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 31 AL0 080H AL1 0 OFS 3
END 

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 156 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER EAGLE 
LABEL XER4
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER7  XEROX 16/8, EM-II (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN XOR1  Xor 5 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,6,2,7,3,8,4,9,5,10
SIDE2 0 1,6,2,7,3,8,4,9,5,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XYZ1  XYZ - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 91 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 2
END 


Diese Formate sind von H.Jungkunz definiert worden f�r 22DISK
Formate in die Datei einbinden und dann indizieren mit
Genindex mydisks.def cpmdisks.def

BEGIN AMS1  Amstrad PCW8256 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS2  Amstrad PCW8256 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS3  Amstrad PCW8256 - SSDD 48 tpi 3" (JOYCE-SYSTEM)
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 07  EXM 0  DSM 174  DRM 63    AL0 0C0H  AL1 0     OFS 1
END

BEGIN AMS4  Amstrad CPC System - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 65,70,66,71,67,72,68,73,69
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMS5  Amstrad CPC-Data - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 193,198,194,199,195,200,196,201,197
BSH 3  BLM 7  EXM 0  DSM 179  DRM 63    AL0 0C0H  AL1 0     OFS 0
END

BEGIN AMS6  Amstrad B360K - SSDD 96 tpi 5.25"  SKEW 2
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 4  BLM 15  EXM 1  DSM 174  DRM 63    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS7  Amstrad VORTEX - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS8  Amstrad CPC System DSDD 96tpi 5.25" - DOBBERTIN -
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN PRO4  Prof80 - IV- DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN SPV1  Spectravideo SV- - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 07  EXM 0  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN TAT1  Tatung  - SSDD 96 tpi 5.25"   (Single sided!)
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SIDE1 0 0,1,2,3,4,5,6,7,8
BSH 4  BLM 15  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

CHWOLKA FORMATE TATUNG1   TATUNG2

SPT                24		24
                   00		00
BLS				   04       04
BLM	               0F		0F
EXT                01		00
DRM                AE		AE
DSM                3F		7F
                   00       00
AL0                80		C0
AL1                










ARK04 +
Z80DOS zu Fritz

24 00 04 0F 01 AE 00 3F 00 80 00 10 00 02 
24 00 04 0F 00 62 01 7F 00 C0 00 20 00 02



NOTE THIS IS THE DATABASE FOR VERSION 1.30 OF 22DISK BY SYDEX.
NOTE Edited JULY 17, 1989  for European Purposes
NOTE     SYDEX
NOTE     153 NORTH MURPHY AVE.
NOTE     SUNNYVALE, CA  94086
NOTE     (408) 739-4866
NOTE ========    Neu dazugekommen bis 2/1992    =====================
NOTE     Rechner                CP/M       Firma
NOTE ----------------------------------------------------------------
NOTE     CPC 664 bis CPC6128    2.2/3.0    Amstrad  /England
NOTE                                       Schneider/Deutschland West
NOTE 
NOTE     PCW8256, PCW8512 &     3.0        Amstrad  /England
NOTE     PCW9512                3.1        Schneider/Deutschland West
NOTE 
NOTE     CPC-/PCW-Hausformate              Dobbertin, Vortex u.a.
NOTE
NOTE     PC1715 & PC1715W       2.2/3.0    Robotron /Deutschland Ost    
NOTE ================================================================

BEGIN A175 PCW8xxx LW A (40*1* 9, 512 1 OFS 2k DIR)   3"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 LABEL A175
BSH 3 BLM 07 EXM 0 DSM 174 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN A195 PCW8xxx LW A (40*1*10, 512 1 OFS 2k DIR)   3 " - Hausformat
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2 
SIDE1 0 1,2,3,4,5,6,7,8,9,10 
LABEL A195 BSH 3 BLM 07 EXM 0 DSM 194 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN A354 PCW8xxx LW B (40*2* 9, 512 1 OFS 8k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A354 BSH 4 BLM 15 EXM 0 DSM 176 DRM 255 AL0 240 AL1 0 OFS 1
END

BEGIN A360 PC1715 IBM & PCW8xxx (40*2* 9, 512 0 OFS 4k DIR) 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A360 BSH 4 BLM 15 EXM 0 DSM 179 DRM 127 AL0 192 AL1 0 OFS 0
END

BEGIN A394 PCW8xxx LW B (40*2*10, 512 1 OFS 4k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 42 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL A394 BSH 4 BLM 15 EXM 0 DSM 206 DRM 127 AL0 192 AL1 0 OFS 1
END

BEGIN A414 PCW8xxx LW B (42*2*10, 512 1 OFS 4k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 42 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL A414 BSH 4 BLM 15 EXM 0 DSM 206 DRM 127 AL0 192 AL1 0 OFS 1
END

BEGIN A714 PCWx512 LW B (80*2* 9, 512 1 OFS 8k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A714 BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END

BEGIN A720 PCW8xxx LW B (81*2* 9, 512 2 OFS 4k DIR)   3-5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 81 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A720 BSH 4 BLM 15 EXM 0 DSM 359 DRM 127 AL0 192 AL1 0 OFS 2
END

BEGIN A780 PC1715 SCP   (80*2* 5,1024 4 OFS 4k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 192 AL1 0 OFS 4
END

BEGIN A800 PC1715 CPA   (80*2* 5,1024 0 OFS 6k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 399 DRM 191 AL0 224 AL1 0 OFS 0
END

BEGIN AMSD CPC Data40   (40*1* 9, 512 0 OFS 2k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SKEW 2 
SIDE1 0 193,198,194,199,195,200,196,201,197 
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN AMSE CPC Data80   (80*1* 9, 512 0 OFS 4k DIR)   5.25"-Hausformat 
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 81,82,83,84,85,86,87,88,89
BSH 4  BLM 15  EXM 2  DSM 178  DRM 127 AL0 0C0H  AL1 0 OFS 0
END

BEGIN AMSS CPC System40 (40*1* 9, 512 2 OFS 2k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMS1 CPC System80 (80*1* 9, 512 2 OFS 2k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 4  BLM 15  EXM 1  DSM 174  DRM 63    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS2 CPC SystemD  (80*2* 9, 512 2 OFS 4k DIR)   5.25"-DOBBERTIN
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73 SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END

BEGIN AMSV VORTEX       (80*2* 9, 512 2 OFS 4k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN MAX3 MAX 3.5"
DENSITY MFM,HIGH CYLINDERS 80 SIDES 2 SECTORS 11,1024 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11 SIDE2 1 1,2,3,4,5,6,7,8,9,10,11 ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 879 DRM 255 AL0 240 AL1 0 OFS 0
END

BEGIN Neue Diskettenformate ENDE ****************************************
DENSITY MFM,LOW CYLINDERS 83 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 176    AL0 255 AL1 0  OFS 0
END

BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 176    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10 LABEL AMI1
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN AMI2  Amigo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL AMI2 BSH 4 BLM 15 EXM 0 DSM 195 DRM 63 AL0 080H AL1 0 OFS 2
END

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN AMP2  Ampro - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26 SIDE2 0 17,18,19,20,21,22,23,24,25,26
ORDER SIDES BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4  BLM 15  EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END

BEGIN AMP4  Ampro - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 17,18,19,20,21 SIDE2 1 17,18,19,20,21
ORDER SIDES BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
END

BEGIN BEE1  Beehive                  - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0 OFS 2
END

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9 SIDE2 1 2,5,8,1,4,7,10,3,6,9 ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN BIG1  BIG BOARD  - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 255    AL0 0C0H  AL1 0     OFS 4
END

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
 ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN CRO2  Cromemco CDOS - DSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
SIDE2 1 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 172  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN CRO4  Cromemco CDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN CRO7  Cromemco CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 1 1,4,7,10,3,6,9,2,5,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 94  DRM 127  AL0 080H     AL1 0    OFS 4
END

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN EC70  ECMA-70 MC-C/PM (10x256) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 3  BLM 07  EXM 00 DSM 143  DRM 63  AL0 0C0H     AL1 0    OFS 4
END

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN EPS3  Epson PX-10 - DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5  BLM 31  EXM 3  DSM 77  DRM 127  AL0 080H     AL1 0    OFS 2
END

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 174  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 172  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4  BLM 15  EXM 1  DSM 82  DRM 95  AL0 0C0H    AL1 0  OFS 3
END

BEGIN HEA2  Heath H89, Magnolia CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 172  DRM 95  AL0 0C0H     AL1 0    OFS 3
END

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 3
END

BEGIN HP1   Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 251  DRM 127  AL0 0F0H     AL1 0    OFS 3
END

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN IBM3  IBM PC, CP/M DSDD 48 tpi 5.25" 8 Sek 0 Offset (REH)
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 0 DSM 157  DRM 63  AL0 080H AL1 0 OFS 0
END


BEGIN ITT2   ITT 3030 CP/M 2.2 DSDD 96 tpi 5.25" 16x256 70 Tracks
DENSITY MFM,LOW
CYLINDERS 70
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 4
END

BEGIN ITT3     ITT3030  CP/M 2.2 DSDD 96 tpi 5.25" 16x256  80 Tracks
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER sides
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 2
END

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 194  DRM 63  AL0 0F0H    AL1 0  OFS 1
END

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 196  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 196  DRM 95  AL0 080H     AL1 0    OFS 2
END

BEGIN KAY4  Kaypro 2X/4/10 - DSDD 48 tpi 5.25" C128 Version
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER sides
BSH 4  BLM 15  EXM 1  DSM 199  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 77
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 299  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 191    AL0 0E0H  AL1 0     OFS 2
END

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 155  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 153  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN NDR1  MC-FLO2  - DSDD 96 tpi 5.25" 1024 Bytes/sec
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END



BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OET1  Oettle & Reichl  - DSDD 96 tpi 5.25"  **** NOT READY !!! ****
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14, 16,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OLI3 Olivetti 250 -  SSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63 AL0 080H    AL1 0  OFS 1
END

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 170  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN OLY3  Olympia ETX 1 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154  DRM 63 AL0 0C0H     AL1 0    OFS 0
END

BEGIN OLY4  Olympia ETX 1 (16x256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154 DRM 63 AL0 080H  AL1 0  OFS 0
END

BEGIN OLY5  Olympia People (16x256 / 2K 128 Dir) - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H     AL1 0    OFS 2
END



BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 45  DRM 63  AL0 080H    AL1 0  OFS 3
END

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 194  DRM 63  AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB9  Osborne Vixen - DSDD 96 tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 392 DRM 255 AL0 0F0H  AL1 0  OFS 6
END

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 311  DRM 127    AL0 0C0H  AL1 0     OFS 4
END


BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN PAR1  PARTNER - CP/M 86 DS HD 96 tpi 5.25"
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3  BLM 7  EXM 0  DSM 151  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN PHI2  Philips PC-2012 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4  BLM 15  EXM 1  DSM 147  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 391  DRM 255    AL0 0F0H  AL1 0     OFS 3
END

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN PRO4  Prof80 - IV- DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN REH1  REH CPU280  5x1024 - DSDD 96 tpi 5.25" 780K Disk
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 399  DRM 255    AL0 0F0H  AL1 0     OFS 0
END

BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 155  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 169  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA2  Sharp MZ-800 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER cylinders
BSH 4  BLM 15  EXM 1 DSM 157  DRM 63   AL0 0C0H  AL1 0     OFS 1
END

BEGIN SHA3  Sharp MZ3500 EOS DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 193 DRM 127  AL0 0F0H  AL1 0     OFS 2
END

BEGIN SHA4  Sharp MZ5600 EOS 16 DSDD 96tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,2,3,4,5
SIDE2 17 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 169  DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA5  Sharp MZ3500 EOS DSDD 48 tpi 5.25"  TESTFORMAT!
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 193 DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SIE1 Siemens  PG-685 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE1
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE2
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN SIE3  Siemens PG-635 DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE3
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE4  Siemens MX 2 (LOC C 25-Format) - DSDD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 192  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 3
END

BEGIN SPV1  Spectravideo SV- - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 07  EXM 0  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN SPY2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 383    AL0 0FCH  AL1 0     OFS 2
END

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 81  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 169  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN TAT1  Tatung  - SSDD 96 tpi 5.25"   (Single sided!)
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SIDE1 0 0,1,2,3,4,5,6,7,8
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TAT2  Tatung  - DSDD 96 tpi 5.25"   (Double sided!)    NOT OKAY!
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 0,3,6,1,4,7,2,5,8
SIDE2 1 0,3,6,1,4,7,2,5,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 153  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 6
END

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 0
SIDES 1
SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3  BLM 7  EXM 0  DSM 71  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 190  DRM 63  AL0 0F0H     AL1 0    OFS 2
END

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN WAV2  Wave Mate Bullet - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 170  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 31  AL0 080H  AL1 0  OFS 3
END

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 7  EXM 0  DSM 156  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
LABEL XER4
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN XER7  XEROX 16/8 (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3  BLM 7  EXM 0  DSM 91  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN2
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN3
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN4
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
LABEL ZEN5
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN6
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL ZEN7
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
LABEL ZEN8
BSH 4  BLM 15  EXM 1  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN NEC3  NEC PC 8801A/8831A - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 152  DRM 127  AL0 0C0H  AL1 0  OFS 4
END



NOTE THIS IS THE DATABASE FOR VERSION 1.30 OF 22DISK BY SYDEX.
NOTE Edited JULY 17, 1989  for European Purposes
NOTE     SYDEX
NOTE     153 NORTH MURPHY AVE.
NOTE     SUNNYVALE, CA  94086
NOTE     (408) 739-4866
NOTE ========    Neu dazugekommen bis 2/1992    =====================
NOTE     Rechner                CP/M       Firma
NOTE ----------------------------------------------------------------
NOTE     CPC 664 bis CPC6128    2.2/3.0    Amstrad  /England
NOTE                                       Schneider/Deutschland West
NOTE 
NOTE     PCW8256, PCW8512 &     3.0        Amstrad  /England
NOTE     PCW9512                3.1        Schneider/Deutschland West
NOTE 
NOTE     CPC-/PCW-Hausformate              Dobbertin, Vortex u.a.
NOTE
NOTE     PC1715 & PC1715W       2.2/3.0    Robotron /Deutschland Ost    
NOTE ================================================================

BEGIN A175 PCW8xxx LW A (40*1* 9, 512 1 OFS 2k DIR)   3"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 LABEL A175
BSH 3 BLM 07 EXM 0 DSM 174 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN A195 PCW8xxx LW A (40*1*10, 512 1 OFS 2k DIR)   3 " - Hausformat
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2 
SIDE1 0 1,2,3,4,5,6,7,8,9,10 
LABEL A195 BSH 3 BLM 07 EXM 0 DSM 194 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN A354 PCW8xxx LW B (40*2* 9, 512 1 OFS 8k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A354 BSH 4 BLM 15 EXM 0 DSM 176 DRM 255 AL0 240 AL1 0 OFS 1
END

BEGIN A360 PC1715 IBM & PCW8xxx (40*2* 9, 512 0 OFS 4k DIR) 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A360 BSH 4 BLM 15 EXM 0 DSM 179 DRM 127 AL0 192 AL1 0 OFS 0
END

BEGIN A394 PCW8xxx LW B (40*2*10, 512 1 OFS 4k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 42 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL A394 BSH 4 BLM 15 EXM 0 DSM 206 DRM 127 AL0 192 AL1 0 OFS 1
END

BEGIN A414 PCW8xxx LW B (42*2*10, 512 1 OFS 4k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 42 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL A414 BSH 4 BLM 15 EXM 0 DSM 206 DRM 127 AL0 192 AL1 0 OFS 1
END

BEGIN A714 PCWx512 LW B (80*2* 9, 512 1 OFS 8k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A714 BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END

BEGIN A720 PCW8xxx LW B (81*2* 9, 512 2 OFS 4k DIR)   3-5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 81 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
LABEL A720 BSH 4 BLM 15 EXM 0 DSM 359 DRM 127 AL0 192 AL1 0 OFS 2
END

BEGIN A780 PC1715 SCP   (80*2* 5,1024 4 OFS 4k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 192 AL1 0 OFS 4
END

BEGIN A800 PC1715 CPA   (80*2* 5,1024 0 OFS 6k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 399 DRM 191 AL0 224 AL1 0 OFS 0
END

BEGIN AMSD CPC Data40   (40*1* 9, 512 0 OFS 2k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SKEW 2 
SIDE1 0 193,198,194,199,195,200,196,201,197 
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN AMSE CPC Data80   (80*1* 9, 512 0 OFS 4k DIR)   5.25"-Hausformat 
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 81,82,83,84,85,86,87,88,89
BSH 4  BLM 15  EXM 2  DSM 178  DRM 127 AL0 0C0H  AL1 0 OFS 0
END

BEGIN AMSS CPC System40 (40*1* 9, 512 2 OFS 2k DIR)   3" - 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMS1 CPC System80 (80*1* 9, 512 2 OFS 2k DIR)   5.25"-Hausformat
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 4  BLM 15  EXM 1  DSM 174  DRM 63    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS2 CPC SystemD  (80*2* 9, 512 2 OFS 4k DIR)   5.25"-DOBBERTIN
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73 SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END

BEGIN AMSV VORTEX       (80*2* 9, 512 2 OFS 4k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN MAX3 MAX 3.5"
DENSITY MFM,HIGH CYLINDERS 80 SIDES 2 SECTORS 11,1024 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11 SIDE2 1 1,2,3,4,5,6,7,8,9,10,11 ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 879 DRM 255 AL0 240 AL1 0 OFS 0
END

BEGIN Neue Diskettenformate ENDE ****************************************

DENSITY MFM,LOW CYLINDERS 83 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 176    AL0 255 AL1 0  OFS 0
END

BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9 SIDE2 1 1,2,3,4,5,6,7,8,9 ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 176    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10 LABEL AMI1
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN AMI2  Amigo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
LABEL AMI2 BSH 4 BLM 15 EXM 0 DSM 195 DRM 63 AL0 080H AL1 0 OFS 2
END

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN AMP2  Ampro - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26 SIDE2 0 17,18,19,20,21,22,23,24,25,26
ORDER SIDES BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4  BLM 15  EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END

BEGIN AMP4  Ampro - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 17,18,19,20,21 SIDE2 1 17,18,19,20,21
ORDER SIDES BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
END

BEGIN BEE1  Beehive                  - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10 SIDE2 1 1,2,3,4,5,6,7,8,9,10 ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0 OFS 2
END

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9 SIDE2 1 2,5,8,1,4,7,10,3,6,9 ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN BIG1  BIG BOARD  - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 255    AL0 0C0H  AL1 0     OFS 4
END

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
 ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN CRO2  Cromemco CDOS - DSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
SIDE2 1 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 172  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN CRO4  Cromemco CDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN CRO7  Cromemco CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 1 1,4,7,10,3,6,9,2,5,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 94  DRM 127  AL0 080H     AL1 0    OFS 4
END

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN EC70  ECMA-70 MC-C/PM (10x256) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 3  BLM 07  EXM 00 DSM 143  DRM 63  AL0 0C0H     AL1 0    OFS 4
END

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN EPS3  Epson PX-10 - DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5  BLM 31  EXM 3  DSM 77  DRM 127  AL0 080H     AL1 0    OFS 2
END

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 174  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 172  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4  BLM 15  EXM 1  DSM 82  DRM 95  AL0 0C0H    AL1 0  OFS 3
END

BEGIN HEA2  Heath H89, Magnolia CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 172  DRM 95  AL0 0C0H     AL1 0    OFS 3
END

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 3
END

BEGIN HP1   Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 251  DRM 127  AL0 0F0H     AL1 0    OFS 3
END

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN IBM3  IBM PC, CP/M DSDD 48 tpi 5.25" 8 Sek 0 Offset (REH)
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 0 DSM 157  DRM 63  AL0 080H AL1 0 OFS 0
END


BEGIN ITT2   ITT 3030 CP/M 2.2 DSDD 96 tpi 5.25" 16x256 70 Tracks
DENSITY MFM,LOW
CYLINDERS 70
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 4
END

BEGIN ITT3     ITT3030  CP/M 2.2 DSDD 96 tpi 5.25" 16x256  80 Tracks
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER sides
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 2
END

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 194  DRM 63  AL0 0F0H    AL1 0  OFS 1
END

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 196  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 196  DRM 95  AL0 080H     AL1 0    OFS 2
END

BEGIN KAY4  Kaypro 2X/4/10 - DSDD 48 tpi 5.25" C128 Version
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER sides
BSH 4  BLM 15  EXM 1  DSM 199  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 77
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 299  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 191    AL0 0E0H  AL1 0     OFS 2
END

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 155  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 153  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN NDR1  MC-FLO2  - DSDD 96 tpi 5.25" 1024 Bytes/sec
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END



BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OET1  Oettle & Reichl  - DSDD 96 tpi 5.25"  **** NOT READY !!! ****
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14, 16,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OLI3 Olivetti 250 -  SSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63 AL0 080H    AL1 0  OFS 1
END

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 170  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN OLY3  Olympia ETX 1 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154  DRM 63 AL0 0C0H     AL1 0    OFS 0
END

BEGIN OLY4  Olympia ETX 1 (16x256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154 DRM 63 AL0 080H  AL1 0  OFS 0
END

BEGIN OLY5  Olympia People (16x256 / 2K 128 Dir) - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H     AL1 0    OFS 2
END



BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 45  DRM 63  AL0 080H    AL1 0  OFS 3
END

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 194  DRM 63  AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB9  Osborne Vixen - DSDD 96 tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 392 DRM 255 AL0 0F0H  AL1 0  OFS 6
END

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 311  DRM 127    AL0 0C0H  AL1 0     OFS 4
END


BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN PAR1  PARTNER - CP/M 86 DS HD 96 tpi 5.25"
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3  BLM 7  EXM 0  DSM 151  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN PHI2  Philips PC-2012 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4  BLM 15  EXM 1  DSM 147  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 391  DRM 255    AL0 0F0H  AL1 0     OFS 3
END

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN PRO4  Prof80 - IV- DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN REH1  REH CPU280  5x1024 - DSDD 96 tpi 5.25" 780K Disk
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 399  DRM 255    AL0 0F0H  AL1 0     OFS 0
END

BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 155  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 169  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA2  Sharp MZ-800 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER cylinders
BSH 4  BLM 15  EXM 1 DSM 157  DRM 63   AL0 0C0H  AL1 0     OFS 1
END

BEGIN SHA3  Sharp MZ3500 EOS DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 193 DRM 127  AL0 0F0H  AL1 0     OFS 2
END

BEGIN SHA4  Sharp MZ5600 EOS 16 DSDD 96tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,2,3,4,5
SIDE2 17 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 169  DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA5  Sharp MZ3500 EOS DSDD 48 tpi 5.25"  TESTFORMAT!
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 193 DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SIE1 Siemens  PG-685 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE1
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE2
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN SIE3  Siemens PG-635 DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE3
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE4  Siemens MX 2 (LOC C 25-Format) - DSDD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 192  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 3
END

BEGIN SPV1  Spectravideo SV- - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 07  EXM 0  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN SPY2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 383    AL0 0FCH  AL1 0     OFS 2
END

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 81  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 169  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN TAT1  Tatung  - SSDD 96 tpi 5.25"   (Single sided!)
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SIDE1 0 0,1,2,3,4,5,6,7,8
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TAT2  Tatung  - DSDD 96 tpi 5.25"   (Double sided!)    NOT OKAY!
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 0,3,6,1,4,7,2,5,8
SIDE2 1 0,3,6,1,4,7,2,5,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 153  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 6
END

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 0
SIDES 1
SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3  BLM 7  EXM 0  DSM 71  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 190  DRM 63  AL0 0F0H     AL1 0    OFS 2
END

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN WAV2  Wave Mate Bullet - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 170  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 31  AL0 080H  AL1 0  OFS 3
END

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 7  EXM 0  DSM 156  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
LABEL XER4
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN XER7  XEROX 16/8 (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3  BLM 7  EXM 0  DSM 91  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN2
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN3
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN4
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
LABEL ZEN5
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN6
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL ZEN7
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
LABEL ZEN8
BSH 4  BLM 15  EXM 1  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 2
END
NOTE    THIS IS THE DATABASE FOR VERSION 1.30 OF 22DISK BY SYDEX.
NOTE
NOTE        Edited JULY 17, 1989  for European Purposes
NOTE
NOTE            SYDEX
NOTE            153 NORTH MURPHY AVE.
NOTE            SUNNYVALE, CA  94086
NOTE            (408) 739-4866



BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 176    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
LABEL AMI1
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN AMI2  Amigo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
LABEL AMI2
BSH 4  BLM 15  EXM 0  DSM 195  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN AMP2  Ampro - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26
SIDE2 0 17,18,19,20,21,22,23,24,25,26
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMP4  Ampro - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 0 17,18,19,20,21
SIDE2 1 17,18,19,20,21
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN AMS1  Amstrad PCW8256 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS2  Amstrad PCW8256 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255    AL0 0F0H  AL1 0     OFS 1
END

BEGIN AMS3  Amstrad PCW8256 - SSDD 48 tpi 3" (JOYCE-SYSTEM)
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 07  EXM 0  DSM 174  DRM 63    AL0 0C0H  AL1 0     OFS 1
END

BEGIN AMS4  Amstrad CPC System - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN AMS5  Amstrad CPC-Data - SSDD 48 tpi 3" or 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201
BSH 3  BLM 7  EXM 0  DSM 179  DRM 63    AL0 0C0H  AL1 0     OFS 0
END

BEGIN AMS6  Amstrad B360K - SSDD 96 tpi 5.25"  SKEW 2
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
BSH 4  BLM 15  EXM 1  DSM 174  DRM 63    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS7  Amstrad VORTEX - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS8  Amstrad CPC System DSDD 96tpi 5.25" - DOBBERTIN -
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 65,66,67,68,69,70,71,72,73
SIDE2 1 65,66,67,68,69,70,71,72,73
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN AMS9  Amstrad DOBBERTIN DATA DSDD 96 tpi 5.25" Skew 5
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201
SIDE2 1 193,194,195,196,197,198,199,200,201
BSH 5  BLM 31  EXM 3  DSM 179  DRM 127   AL0 080H  AL1 0     OFS 0
END

BEGIN AMSA  Amstrad PCW8256 - DSDD 96 tpi 5.25" 10 x 512 788K
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
LABEL AMSA
BSH 5  BLM 31  EXM 3  DSM 197  DRM 255    AL0 0C0H  AL1 0     OFS 1
END

BEGIN BEE1  Beehive - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
SIDE2 1 2,5,8,1,4,7,10,3,6,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN BIG1  BIG BOARD  - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 255    AL0 0C0H  AL1 0     OFS 4
END

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CMX   CMX EDIT SYSTEM  - DSDD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL IBM2
BSH 4  BLM 15  EXM 0  DSM 350  DRM 127 AL0 0C0H     AL1 0    OFS 2
END

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN CRO2  Cromemco CDOS - DSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
SIDE2 1 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 172  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN CRO4  Cromemco CDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN CRO7  Cromemco CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 1 1,4,7,10,3,6,9,2,5,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 94  DRM 127  AL0 080H     AL1 0    OFS 4
END

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN EC70  ECMA-70 MC-C/PM (10x256) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 3  BLM 07  EXM 00 DSM 143  DRM 63  AL0 0C0H     AL1 0    OFS 4
END

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN EPS3  Epson PX-10 - DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 139  DRM 63  AL0 080H     AL1 0    OFS 8
END

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5  BLM 31  EXM 3  DSM 77  DRM 127  AL0 080H     AL1 0    OFS 2
END

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 174  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 172  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4  BLM 15  EXM 1  DSM 82  DRM 95  AL0 0C0H    AL1 0  OFS 3
END

BEGIN HEA2  Heath H89, Magnolia CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 172  DRM 95  AL0 0C0H     AL1 0    OFS 3
END

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 3
END

BEGIN HP1   Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 251  DRM 127  AL0 0F0H     AL1 0    OFS 3
END

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN IBM3  IBM PC, CP/M DSDD 48 tpi 5.25" 8 Sek 0 Offset (REH)
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
LABEL IBM2
BSH 4  BLM 15  EXM 0 DSM 157  DRM 63  AL0 080H AL1 0 OFS 0
END


BEGIN ITT2   ITT 3030 CP/M 2.2 DSDD 96 tpi 5.25" 16x256 70 Tracks
DENSITY MFM,LOW
CYLINDERS 70
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 4
END

BEGIN ITT3     ITT3030  CP/M 2.2 DSDD 96 tpi 5.25" 16x256  80 Tracks
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER sides
BSH 4  BLM 15  EXM 0 DSM 271 DRM 127  AL0 0C0H AL1 0 OFS 2
END

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 194  DRM 63  AL0 0F0H    AL1 0  OFS 1
END

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 196  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 196  DRM 95  AL0 080H     AL1 0    OFS 2
END

BEGIN KAY4  Kaypro 2X/4/10 - DSDD 48 tpi 5.25" C128 Version
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER sides
BSH 4  BLM 15  EXM 1  DSM 199  DRM 63  AL0 0C0H     AL1 0    OFS 1
END

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 77
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 299  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 191    AL0 0E0H  AL1 0     OFS 2
END

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 155  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 153  DRM 127    AL0 0C0H  AL1 0     OFS 3
END

BEGIN NDR1  MC-FLO2  - DSDD 96 tpi 5.25" 1024 Bytes/sec
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN NEC3  NEC PC 8801A/8831A - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 152  DRM 127  AL0 0C0H  AL1 0  OFS 4
END

BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OET1  Oettle & Reichl  - DSDD 96 tpi 5.25"  **** NOT READY !!! ****
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 176  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14, 16,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OLI3 Olivetti 250 -  SSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 4  BLM 15  EXM 1  DSM 157  DRM 63 AL0 080H    AL1 0  OFS 1
END

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3  BLM 7  EXM 0  DSM 170  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN OLY3  Olympia ETX 1 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154  DRM 63 AL0 0C0H     AL1 0    OFS 0
END

BEGIN OLY4  Olympia ETX 1 (16x256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3  BLM 7  EXM 0 DSM 154 DRM 63 AL0 080H  AL1 0  OFS 0
END

BEGIN OLY5  Olympia People (16x256 / 2K 128 Dir) - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H     AL1 0    OFS 2
END



BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 45  DRM 63  AL0 080H    AL1 0  OFS 3
END

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 184  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 189  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 389  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 194  DRM 63  AL0 0C0H  AL1 0     OFS 2
END

BEGIN OSB9  Osborne Vixen - DSDD 96 tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 392 DRM 255 AL0 0F0H  AL1 0  OFS 6
END

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 311  DRM 127    AL0 0C0H  AL1 0     OFS 4
END


BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN PAR1  PARTNER - CP/M 86 DS HD 96 tpi 5.25"
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 4
END


BEGIN PCPM  IBM PC, PCP/M-86 - DSDD 96 tpi 5.25" 720K
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL IBM2
BSH 4  BLM 15  EXM 0  DSM 350  DRM 127 AL0 0C0H     AL1 0    OFS 4
END

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3  BLM 7  EXM 0  DSM 151  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN PHI2  Philips PC-2012 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 157  DRM 127    AL0 080H  AL1 0     OFS 2
END

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4  BLM 15  EXM 1  DSM 147  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 391  DRM 255    AL0 0F0H  AL1 0     OFS 3
END

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN PRO4  Prof80 - IV- DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 1
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 384  DRM 127    AL0 0C0H  AL1 0     OFS 6
END

BEGIN REH1  REH CPU280  5x1024 - DSDD 96 tpi 5.25" 780K Disk
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0 DSM 399  DRM 255    AL0 0F0H  AL1 0     OFS 0
END

BEGIN REH2  REH CPU280  9x1024 - HD 96 tpi 5.25" 1.432K Disk
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SKEW 2
SECTORS 9,1024
SIDE1 0 1,3,5,7,9,2,4,6,8
SIDE2 1 1,3,5,7,9,2,4,6,8
ORDER SIDES
BSH 5  BLM 31  EXM 1 DSM 359  DRM 255 AL0 0C0H   AL1 0    OFS 0
END

BEGIN REH3  REH CPU280 11x1024 - HD 135 tpi 3.5" 1770K Disk
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SECTORS 11,1024
SIDE1 0 1,3,5,7,9,11,2,4,6,8,10
SIDE2 1 1,3,5,7,9,11,2,4,6,8,10
ORDER SIDES
BSH 5  BLM 31  EXM 1 DSM 439  DRM 255 AL0 0C0H   AL1 0    OFS 0
END

BEGIN REH4  REH CPU280 11x1024 - HD 135 tpi 3.5" 1770K Disk  Track 0 bad
DENSITY MFM,HIGH
CYLINDERS 80
SIDES 2
SKEW 1
SECTORS 11,1024
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11
ORDER SIDES
BSH 5  BLM 31  EXM 1 DSM 439  DRM 255 AL0 0C0H   AL1 0    OFS 1
END


NOTE   Robotron Formate 780K  und 800K

BEGIN R780 PC1715 SCP   (80*2* 5,1024 4 OFS 4k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 192 AL1 0 OFS 4
END

BEGIN R800 PC1715 CPA   (80*2* 5,1024 0 OFS 6k DIR)   5.25"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
SIDE1 0 1,2,3,4,5 SIDE2 1 1,2,3,4,5 ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 399 DRM 191 AL0 224 AL1 0 OFS 0
END


BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 151  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN ROY2  Royal Alphatronic P2 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 07  EXM 0  DSM 151  DRM 64   AL0 0C0H  AL1 0     OFS 2
END

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 315  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 155  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 155  DRM 127    AL0 080H  AL1 0     OFS 4
END

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 169  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA2  Sharp MZ-800 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER cylinders
BSH 4  BLM 15  EXM 1 DSM 157  DRM 63   AL0 0C0H  AL1 0     OFS 1
END

BEGIN SHA3  Sharp MZ3500 EOS DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 193 DRM 127  AL0 0F0H  AL1 0     OFS 2
END

BEGIN SHA4  Sharp MZ5600 EOS 16 DSDD 96tpi 5.25" 5x1024
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,2,3,4,5
SIDE2 17 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 169  DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SHA5  Sharp MZ3500 EOS DSDD 48 tpi 5.25"  TESTFORMAT!
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 2
SIDE1 16 1,3,5,2,4
SIDE2 17 1,3,5,2,4
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 193 DRM 127  AL0 0C0H  AL1 0     OFS 2
END

BEGIN SIE1 Siemens  PG-685 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE1
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE2
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN SIE3  Siemens PG-635 DSDD 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
LABEL SIE3
BSH 4  BLM 15  EXM 0  DSM 350  DRM 255    AL0 0F0H  AL1 0     OFS 4
END

BEGIN SIE4  Siemens MX 2 (LOC C 25-Format) - DSDD 96 tpi 3.5"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 192  DRM 127    AL0 0C0H  AL1 0     OFS 4
END

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 3
END

BEGIN SPV1  Spectravideo SV- - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 07  EXM 0  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN SPV2  Spectravideo SV- - SSDD 96 tpi 3.5" Dr. Eberl vermutlich!
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15  EXM 1  DSM 172  DRM 63  AL0 080H     AL1 0    OFS 3
END


BEGIN SPY2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 383    AL0 0FCH  AL1 0     OFS 2
END

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 81  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 63  AL0 080H    AL1 0  OFS 2
END

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
COMPLEMENT
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 169  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN TAT1  Tatung  - SSDD 96 tpi 5.25"   (Single sided!)
DENSITY MFM,LOW
CYLINDERS 80
SIDES 1
SECTORS 9,512
SIDE1 0 0,1,2,3,4,5,6,7,8
BSH 4  BLM 15  EXM 1  DSM 170  DRM 63    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TAT2  Tatung  - DSDD 96 tpi 5.25"   (Double sided!)    NOT OKAY!
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 0,3,6,1,4,7,2,5,8
SIDE2 1 0,3,6,1,4,7,2,5,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS
BSH 4  BLM 15  EXM 0  DSM 153  DRM 63  AL0 080H     AL1 0    OFS 1
END

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 354  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES
BSH 3  BLM 7  EXM 0  DSM 255  DRM 63  AL0 0C0H    AL1 0  OFS 6
END

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 0
SIDES 1
SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3  BLM 7  EXM 0  DSM 71  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3  BLM 7  EXM 0  DSM 170  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 190  DRM 63  AL0 0F0H     AL1 0    OFS 2
END

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4  BLM 15  EXM 1  DSM 94  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4  BLM 15  EXM 1  DSM 84  DRM 127  AL0 0C0H     AL1 0    OFS 2
END

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 174  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3  BLM 7  EXM 0  DSM 155  DRM 63  AL0 0C0H    AL1 0  OFS 1
END

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3  BLM 7  EXM 0  DSM 189  DRM 63  AL0 0C0H    AL1 0  OFS 2
END

BEGIN WAV2  Wave Mate Bullet - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 394  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS
BSH 4  BLM 15  EXM 1  DSM 170  DRM 127    AL0 0C0H  AL1 0     OFS 2
END

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3  BLM 7  EXM 0  DSM 82  DRM 31  AL0 080H  AL1 0  OFS 3
END

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3  BLM 7  EXM 0  DSM 156  DRM 63  AL0 0C0H    AL1 0  OFS 3
END

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS
LABEL XER4
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 0C0H     AL1 0    OFS 3
END

BEGIN XER7  XEROX 16/8 (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 162  DRM 63  AL0 080H     AL1 0    OFS 4
END

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM,LOW
CYLINDERS 40
SIDES 1
SECTORS 10,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3  BLM 7  EXM 0  DSM 91  DRM 63  AL0 0C0H  AL1 0  OFS 3
END

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN2
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN3
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN4
BSH 4  BLM 15  EXM 0  DSM 315  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
LABEL ZEN5
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES
LABEL ZEN6
BSH 4  BLM 15  EXM 0  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL ZEN7
BSH 3  BLM 7  EXM 0  DSM 151  DRM 127  AL0 0F0H     AL1 0    OFS 2
END

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES
LABEL ZEN8
BSH 4  BLM 15  EXM 1  DSM 155  DRM 255    AL0 0F0H  AL1 0     OFS 2
END

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 1  DSM 194  DRM 63  AL0 080H     AL1 0    OFS 2
END

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM,LOW
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 5  BLM 31  EXM 3  DSM 194  DRM 127    AL0 080H  AL1 0     OFS 2
END

