NOTE 	THIS IS THE DATABASE FOR VERSION 1.40 OF 22DISK BY SYDEX.
NOTE 
NOTE 			SYDEX
NOTE 			P.O. Box 5700
NOTE 			Eugene, OR  97405
NOTE 			(503) 683-6033

BEGIN A1  Generic CP/M - SSSD 8"
DENSITY FM ,HIGH CYLINDERS 77 SIDES 1 SECTORS 26,128
SIDE1 0 1,7,13,19,25,5,11,17,23,3,9,15,21,2,8,14,20,26,6,12,18,24,4,10,16,22
BSH 3 BLM 7 EXM 0 DSM 242 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABC1  ABC-80 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 16,256
SIDE1 0 1,8,15,6,13,4,11,2,9,16,7,14,5,12,3,10
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ABD1  A. B. Dick Magna III - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 2 SECTORS 16,256 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 0 17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 255 AL0 0FFH AL1 0 OFS 4
END 

BEGIN ACT1  Actrix (Access Matrix) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADL1  Adler Textriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN ADV1  Advanced Digital Super 6 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 4,1024
SIDE1 0 1,2,3,4
BSH 4 BLM 15 EXM 0 DSM 77 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN ADV3  Advanced Digital Super 6 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 4,1024
SKEW 2
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 300 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ADV5  Advanced Digital TurboDOS 312K - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 0 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ALT5  Altos Series 5 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 176 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMI1  Amigo - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN AMP3  Ampro - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SKEW 2
SIDE1 0 1,2,3,4,5
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AMS1  Amstrad PCW8256 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4 BLM 15 EXM 0 DSM 356 DRM 255 AL0 0F0H AL1 0 OFS 1
END 

BEGIN AMSD  Amstrad PCW 9256, 9512 Disckit - DSDD 3.5"
SEE AMS1

BEGIN ARC1  Archive I - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN ARC2  Archive II & III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES EVEN-ODD 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 319 AL0 0F8H AL1 0 OFS 2
END 

BEGIN ARI1  Arisia - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 147 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ATR1  ATR-8000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SKEW 3
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN AVA1  Avatar - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 1,5,9,3,7,2,6,10,4,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BEE1  Beehive - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BEE2  Beehive Microbee - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 2,5,8,1,4,7,10,3,6,9
SIDE2 1 2,5,8,1,4,7,10,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BIT1  Bitelex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 131 DRM 95 AL0 0E0H AL1 0 OFS 2
END 

BEGIN BMC1  BMC IF800 Model 20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,7,13,19,5,11,17,3,9,15
SIDE2 1 1,7,13,19,5,11,17,3,9,15
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN BON1  Bondwell 12 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BON2  Bondwell 14 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN BUR1  Burr-Brown - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
SIDE2 1 1,10,2,11,3,12,4,13,5,14,6,15,7,16,8,17,9,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN CAL1  Cal-PC - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS1  Cashcom 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 303 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CAS2  Casio FP-1100/FP-1020 - DSDD 48tpi 5.25"
SEE FUJ2

BEGIN CCS1  CCS (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
SIDE2 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 165 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS2  CCS (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,4,7,10,3,6,9,2,5,8
SIDE2 0 1,4,7,10,3,6,9,2,5,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CCS3  CCS (1024 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 0 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 184 DRM 63 AL0 080H AL1 0 OFS 6
END 

BEGIN CDI1  CDI-5000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN CMC1  CMC Supersystem 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN COL1  Coleco ADAM, 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,6,3,8,5,2,7,4
BSH 3 BLM 7 EXM 0 DSM 146 DRM 63 AL0 0C0H AL1 0 SOFS 26
END 

BEGIN COM1  Compis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 317 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM2  Compugraphic MCS-5 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN COM3  Compustar Model 30 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN COM4  Compupro (Viasyn) (1024 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN CRO1  Cromemco CDOS - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,128 SKIP 
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN CRO3  Cromemco CDOS - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512 SKIP 
SIDE1 0 1,5,9,3,7,2,6,10,4,8
LABEL CRO3
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CRO6  Cromemco CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512 SKIP 
SIDE1 0 1,4,7,10,3,6,9,2,5,8
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CWP1  C/WP Cortex - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN CYK1  Cykey - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DAT1  Datavue DV80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 129,130,131,132,133,134,135,136,137,138
SIDE2 1 129,130,131,132,133,134,135,136,137,138
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 94 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DAT2  Datavue DV80 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 1 193,194,195,196,197,198,199,200,201,202
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN DEC1  DEC DECMate II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DEC2  DEC Rainbow - SSDD 96 tpi 5.25"
SEE DEC1

BEGIN DEC3  DEC VT-180 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SIDE1 0 1,3,5,7,9,2,4,6,8
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN DIG1  Digilog - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 0 1,2,3,4,5
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 166 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN DIG2  Digilog 1500 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 392 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIR1  Direct 1025 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 152 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN DIS1  Discovery - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 313 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN EAG1  Eagle II - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN EAG2  Eagle III - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 394 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN EPS1  Epson QX-10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN EPS2  Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN EPS3  Epson PX-8 - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 139 DRM 63 AL0 080H AL1 0 OFS 8
END 

BEGIN ERI1  Ericsson DTC - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 5 BLM 31 EXM 3 DSM 77 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI2  Ericsson DTC2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN ERI3  Ericsson Step One - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 174 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN FLO1  Florida Graphics - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
SIDE2 1 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 295 DRM 127 AL0 0C0H AL1 0 OFS 12
END 

BEGIN FOR1  Formula 1 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN FUJ1  Fujitsu Micro 16 - DSDD 48 tpi 5.25"
SEE IBM2

BEGIN FUJ2  Fujitsu Micro 8 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN GNA1  Gnat System 10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HCL1  HCL System 2 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN HEA1  Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 4 BLM 15 EXM 1 DSM 82 DRM 95 AL0 0C0H AL1 0 OFS 3
END 

BEGIN HEA3  Heath H89, Magnolia CP/M - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 3
END 

BEGIN HEU1  Heurikon MLZ-91A - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
SIDE2 1 1,2,5,6,9,10,13,14,3,4,7,8,11,12,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN HP1  Hewlett-Packard HP 86, 87, 125 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
SIDE2 1 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 251 DRM 127 AL0 0F0H AL1 0 OFS 3
END 

BEGIN IBM1  IBM PC, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
LABEL IBM1
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN IBM2  IBM PC, CP/M-86 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
LABEL IBM2
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN IMS1  IMS 5000 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,9,2,10,3,11,4,12,5,13,6,14,7,15,8,16
BSH 3 BLM 7 EXM 0 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN IMS2  IMS 5000 TurboDOS - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 380 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN INT1  Intel iPDS 100 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 307 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN INS1  Insight Enterprises - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ITH1  Ithaca Intersystems - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 1,2,5,6,9,10,13,14,17,18,3,4,7,8,11,12,15,16
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN JET1  Jet-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN KAY1  Kaypro II/2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 194 DRM 63 AL0 0F0H AL1 0 OFS 1
END 

BEGIN KAY2  Kaypro 2X/4/10 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 196 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN KAY3  Kaypro, Pro-8 ROM - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 0 20,21,22,23,24,25,26,27,28,29
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 196 DRM 95 AL0 080H AL1 0 OFS 2
END 

BEGIN KON1  Kontron - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 77
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 299 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN LEX1  Lexoriter - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 3 BLM 7 EXM 0 DSM 159 DRM 31 AL0 080H AL1 0 OFS 0
END 

BEGIN LOB1  Lobo Max-80 (256 bytes/sector) - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 165 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB3  Lobo Max-80 (512 bytes/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN LOB4  Lobo Max-80 (512 bytes/sector) - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 0,1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN LNW1  LNW 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 4 BLM 15 EXM 1 DSM 82 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MAC1  Macsym 150 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MAG1  Magic - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN MAI1  MAI Basic Four - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 312 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN MIC2  Micromint SB180 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 17,18,19,20,21,22,23,24,25,26
SIDE2 1 17,18,19,20,21,22,23,24,25,26
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MIC3  Micron Quark - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MIC5  Micro Source M6000 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 0 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MOL1  Molecular Series 9 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 179 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MOL2  Molecular/Durango Poppy 54 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 3
SIDE1 0 128,129,130,131,132,133,134,135,136,137
SIDE2 1 138,139,140,141,142,143,144,145,146,147
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN MON1  Monroe 8800 Series - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
BSH 4 BLM 15 EXM 1 DSM 153 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN MOR1  Morrow MD2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN MOR2  Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,4,2,5,3
SIDE2 1 1,4,2,5,3
ORDER SIDES LABEL MOR2
BSH 4 BLM 15 EXM 1 DSM 194 DRM 191 AL0 0E0H AL1 0 OFS 2
END 

BEGIN MOR6  Morrow TurboDOS - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 4,1024
SIDE1 0 1,2,3,4
SIDE2 1 1,2,3,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN NCR1  NCR Decision Mate V - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 153 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN NCR2  NCR FirstStep - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 276 DRM 255 AL0 0F0H AL1 0 OFS 6
END 

BEGIN NEC1  NEC PC-8001A - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN NEC3  NEC PC 8801A/8831A - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 152 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NEC4  NEC PC 8500/8431A, Starlet - DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN NIA1  Niat - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER CYLINDERS 
BSH 5 BLM 31 EXM 3 DSM 157 DRM 127 AL0 080H AL1 0 OFS 2
END 

BEGIN NIX1  Nixdorf 8810/30 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN OKI1  OKI IF800 Model 20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,7,13,19,5,11,17,3,9,15
SIDE2 1 1,7,13,19,5,11,17,3,9,15
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OLI1  Olivetti ETV300 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14, 16,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OLI2  Olivetti M20 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OLI3  Olivetti 250 -  SSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 4 BLM 15 EXM 1 DSM 157 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN OLY1  Olympia EX-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OLY2  Olympia ETX II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN OSB1  Osborne 1 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,256
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 45 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN OSB2  Osborne 1 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 184 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OSB3  Osborne Executive - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 184 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OSB4  Osborne G2 System - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 189 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OSB5  Osborne G2 System - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SKEW 1
SIDE1 0 1,2,3,4,5
SIDE2 1 6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 389 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN OSB6  Osborne 1 + Osmosis - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 384 DRM 127 AL0 0C0H AL1 0 OFS 6
END 

BEGIN OSB7  Osborne Nuevo - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 6,8,10,7,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB8  Osborne Vixen - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN OSB9  Osborne Executive w/Z3 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 5,1024
SIDE1 0 1,3,5,2,4
SIDE2 1 1,3,5,2,4
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 395 DRM 127 AL0 0F8H AL1 0 OFS 2
END 

BEGIN OSM1  OSM Zeus 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 311 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN OTR1  Otrona Attache - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER EAGLE 
BSH 4 BLM 15 EXM 1 DSM 181 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN OTR2  Otrona Attache - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 386 DRM 127 AL0 0C0H AL1 00H OFS 3
END 

BEGIN PAN1  Panasonic KX-E828 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN PEG1  Pegasus Data Logger - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,4,7,2,5,8,3,6,9
SIDE2 1 1,4,7,2,5,8,3,6,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 80H AL1 0 OFS 6
END 

BEGIN PHI1  Philips PC-2010 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SIDE1 0 1,3,5,7,9,11,13,15,2,4,6,8,10,12,14,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PHI3  Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
BSH 4 BLM 15 EXM 1 DSM 147 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN PIE1  Pied Piper - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 391 DRM 255 AL0 0F0H AL1 0 OFS 3
END 

BEGIN PMC1  PMC Micromate - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
SIDE2 1 1,2,3,4,5
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN PRO2  Proglas 770KB - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 388 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN ROY1  Royal Alphatronic - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 1
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 151 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN SAG1  Sage IV - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAG2  Sage IV - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN1  Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SAN2  Sanyo  MBC-1250 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
SIDE2 1 1,4,7,10,13,16,3,6,9,12,15,2,5,8,11,14
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 155 DRM 127 AL0 080H AL1 0 OFS 4
END 

BEGIN SEE1  Seequa Chameleon - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN SEI1  Seiko - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SHL1  Shelton SIG/NET 2 - SSDD 48 tpi 5.25"
SEE SUP2

BEGIN SHA1  Sharp MZ-80 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10
SIDE2 0 1,2,3,4,5,6,7,8,9,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN SIE1  Siemens  PG-685 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SIE2  Siemens PG-675 DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN SIE3  Siemens PG-635 DSDD 3.5"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 350 DRM 255 AL0 0F0H AL1 0 OFS 4
END 

BEGIN SOR1  Sorbus TurboDOS - 5.25" DSHD (or 8" DSDD)
DENSITY MFM ,HIGH 
CYLINDERS 77
SIDES 2
SECTORS 8,1024
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 5 BLM 31 EXM 1 DSM 308 DRM 255 AL0 0C0H AL1 0 OFS 0
END 

BEGIN SPE1  Spectravideo SV-328 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 2
SIDE1 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 3
END 

BEGIN SPE2  Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 383 AL0 0FCH AL1 0 OFS 2
END 

BEGIN SUP1  Superbrain JR - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 81 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP2  Superbrain 40 track - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SUP3  Superbrain QD - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
COMPLEMENT 
CYLINDERS 35
SIDES 2
SECTORS 10,512
SIDE1 0 1,3,5,7,9,2,4,6,8,10
SIDE2 1 1,3,5,7,9,2,4,6,8,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 169 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN SYS2  Systel 2 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
BSH 3 BLM 7 EXM 0 DSM 170 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN SYS3  Systel 3 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TEK1  Tektronix 4170 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 0 DSM 153 DRM 63 AL0 080H AL1 0 OFS 1
END 

BEGIN TEL2  Teletek Systemaster - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
SIDE2 1 1,7,13,2,8,14,3,9,15,4,10,16,5,11,17,6,12,18
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 172 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TEL3  Televideo 801, 806 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SKEW 6
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END 

BEGIN TEL4  Televideo 1603 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 354 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TI1  TI Professional, CP/M-86 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TOS1  Toshiba T100, T200 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
SIDE2 1 1,5,9,13,2,6,10,14,3,7,11,15,4,8,12,16
ORDER SIDES 
BSH 3 BLM 7 EXM 0 DSM 255 DRM 63 AL0 0C0H AL1 0 OFS 6
END 

BEGIN TRS1  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 0
SIDES 1
SECTORS 18,128
SIDE1 0 1,5,9,13,17,3,7,11,15,2,6,10,14,18,4,8,12,16
BSH 3 BLM 7 EXM 0 DSM 71 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN TRS3  TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SKEW 5
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS7  TRS-80, Holmes CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 4
SIDE1 0 0,1,2,3,4,5,6,7,8,9
SIDE2 1 10,11,12,13,14,15,16,17,18,19
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 190 DRM 63 AL0 0F0H AL1 0 OFS 2
END 

BEGIN TRS8  TRS-80, MM CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRS9  TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
BSH 4 BLM 15 EXM 1 DSM 84 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSA  TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 18,256
SIDE1 0 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
SIDE2 1 1,3,5,7,9,11,13,15,17,2,4,6,8,10,12,14,16,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 174 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN TRSB  TRS-80 Model 4 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SKEW 4
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END 

BEGIN TRSC  TRS-80 Model 3, Hurricane CP/M - SSDD 48 tpi 5.25"
SEE MOR1

BEGIN VEC1  Vector 4 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER EAGLE 
BSH 4 BLM 15 EXM 0 DSM 356 DRM 127 AL0 0C0H AL1 0 OFS 1
END 

BEGIN VIS1  Visual 1050 - SSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 1
SECTORS 10,512
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAN1  Wangwriter - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN WAV1  Wave Mate Bullet - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 5,1024
SIDE1 0 1,2,3,4,5
BSH 3 BLM 7 EXM 0 DSM 189 DRM 63 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER1  Xerox (512 byte/sector) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 170 DRM 127 AL0 0C0H AL1 0 OFS 2
END 

BEGIN XER2  Xerox 820 - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 18,128
SIDE1 0 1,6,11,16,3,8,13,18,5,10,15,2,7,12,17,4,9,14
BSH 3 BLM 7 EXM 0 DSM 82 DRM 31 AL0 080H AL1 0 OFS 3
END 

BEGIN XER3  Xerox 820 II - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
BSH 3 BLM 7 EXM 0 DSM 156 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER4  Xerox 820-II and 16/8 (EM II) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 17,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17
ORDER EAGLE 
LABEL XER4
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XER7  XEROX 16/8, EM-II (Standalone) - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 9,512
SKEW 2
SIDE1 240 1,2,3,4,5,6,7,8,9
SIDE2 242 1,2,3,4,5,6,7,8,9
ORDER CYLINDERS 
BSH 4 BLM 15 EXM 1 DSM 162 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN XOR1  Xor 5 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,6,2,7,3,8,4,9,5,10
SIDE2 0 1,6,2,7,3,8,4,9,5,10
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 191 DRM 127 AL0 0C0H AL1 0 OFS 3
END 

BEGIN XYZ1  XYZ - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SIDE1 0 1,5,9,3,7,2,6,10,4,8
SIDE2 1 11,15,19,13,17,12,16,20,14,18
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 4
END 

BEGIN ZEN1  Zenith Z-37 Disk - SSSD 48 tpi 5.25"
DENSITY FM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 10,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10
BSH 3 BLM 7 EXM 0 DSM 91 DRM 63 AL0 0C0H AL1 0 OFS 3
END 

BEGIN ZEN2  Zenith Z-37 Disk - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN3  Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN4  Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 315 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN5  Zenith Z90 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN6  Zenith Z90 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 16,256
SKEW 3
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16
ORDER SIDES 
BSH 4 BLM 15 EXM 0 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 1
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
BSH 3 BLM 7 EXM 0 DSM 151 DRM 127 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 8,512
SIDE1 0 1,2,3,4,5,6,7,8
SIDE2 1 1,2,3,4,5,6,7,8
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 155 DRM 255 AL0 0F0H AL1 0 OFS 2
END 

BEGIN ZOR1  Zorba - DSDD 48 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 40
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 4 BLM 15 EXM 1 DSM 194 DRM 63 AL0 080H AL1 0 OFS 2
END 

BEGIN ZOR2  Zorba - DSDD 96 tpi 5.25"
DENSITY MFM ,LOW 
CYLINDERS 80
SIDES 2
SECTORS 10,512
SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES 
BSH 5 BLM 31 EXM 3 DSM 194 DRM 127 AL0 080H AL1 0 OFS 2
END 

