NOTE    THIS IS a DATABASE FOR VERSION 1.38 OF 22DISK BY SYDEX.
note
note  Last update: 28.3.1994
note  ----------------------
note  skip = initial tracks in Single Density
note  order sides even-odd = ???;  order eagle !
note  see = ?? (cross reference)

BEGIN V1  Vortex - DSDD 96 tpi 5.25 - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
SIDE2 1 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
ORDER SIDES
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END

BEGIN AS4  Amstrad CPC 249K System 53 tracks Side 2
note only 3,5" and 5,25" drive
DENSITY MFM,LOW CYLINDERS 106 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 250 DRM 63 AL0 0C0H AL1 0 OFS 108
END

BEGIN AS3  Amstrad CPC 249K System 53 tracks Side 1
note only 3,5" and 5,25" drive
DENSITY MFM,LOW CYLINDERS 106 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 250 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN MAD1  Amstrad CPC 253K 56 pistes System Side 1
DENSITY MFM,LOW CYLINDERS 114 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 254 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN MAD2  Amstrad CPC 253K 56 pistes System Side 2
DENSITY MFM,LOW CYLINDERS 114 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 254 DRM 63 AL0 0C0H AL1 0 OFS 116
END

BEGIN MADD  Amstrad CPC MADRAM 249K System 53 tracks Side 1
note only DD 3,5" and 5,25" drive
DENSITY MFM,LOW CYLINDERS 106 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 046h, 042h, 047h, 043h, 048h, 044h, 049h, 045h
BSH 3 BLM 7 EXM 0 DSM 250 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN AS2b  Amstrad CPC 169K System Side 2 en 5,25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 42
END

BEGIN AS1b  Amstrad CPC 169K System Side 1 en 5,25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN MAD2  Amstrad CPC 253K System Side 2 en 5,25"
DENSITY MFM,LOW CYLINDERS 60 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 046h, 042h, 047h, 043h, 048h, 044h, 049h, 045h
SIDE2 0 041h, 046h, 042h, 047h, 043h, 048h, 044h, 049h, 045h
ORDER eagle
BSH 3 BLM 7 EXM 0 DSM 254 DRM 63 AL0 0C0H AL1 0 OFS 62
END

BEGIN MAD1  Amstrad CPC 253K System Side 1 en 5,25"
DENSITY MFM,LOW CYLINDERS 60 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 046h, 042h, 047h, 043h, 048h, 044h, 049h, 045h
BSH 3 BLM 7 EXM 0 DSM 254 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN AS2  Amstrad CPC 169K System Side 2 en 3,5"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 82
END

BEGIN AS1  Amstrad CPC 169K System Side 1 en 3,5"
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN AD4  Amstrad CPC 187K DATA 42 tracks Side 2 en 3,5"
DENSITY MFM,LOW CYLINDERS 84 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 188 DRM 63 AL0 0C0H AL1 0 OFS 42
END

BEGIN AD3  Amstrad CPC 187K DATA 42 tracks Side 1 en 3,5"
DENSITY MFM,LOW CYLINDERS 84 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 188 DRM 63 AL0 0c0H AL1 0 OFS 0
END

BEGIN AD2b  Amstrad CPC 178K Data Side 2 en 5,25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 40
END

BEGIN AD1b  Amstrad CPC 178K Data Side 1 en 5,25"
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0c0H AL1 0 OFS 0
END

BEGIN AD2  Amstrad CPC 178K Data Side 2 en 3,5"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 80
END

BEGIN AD1  Amstrad CPC 178K Data Side 1 en 3,5"
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0c0H AL1 0 OFS 0
END

BEGIN AI2  Amstrad CPC 154K IBM CP/M-86 SSDD Side 2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
SIDE2 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 41
END

BEGIN AI1  Amstrad CPC 154K IBM CP/M-86 SSDD Side 1
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END


BEGIN KCS1  KC Compact 169K System Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN KCD1  KC Compact 178K Data Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN P2  Amstrad PCW8256 - DSDD 48 tpi - 9x512x40x2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN P1  Amstrad PCW8256 - DSDD 96tpi - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN AP2  Amstrad CPC DiskPara 3-Format DSDD 96tpi 10x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 399  DRM 127  AL0 0C0H  AL1 0  OFS 0
END

BEGIN AP1  Amstrad CPC 830K-DiskPara-Format - DDSS 10x512x83x2
DENSITY MFM,LOW CYLINDERS 83 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 414  DRM 191  AL0 224  AL1 0  OFS 0
END

BEGIN MAG1 MAGIC DOS from longshot (Serge Querne) 2x410Ko DSDD side 1
DENSITY MFM,LOW CYLINDERS 82 SIDES 1 SECTORS 10,512 SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201,202
ORDER CYLINDERS
BSH 004h BLM 00fh EXM 001h DSM 0cch DRM 03fh AL0 080h AL1 000h OFS 000h
END

BEGIN MAG2 MAGIC DOS from longshot (Serge Querne) 2x410Ko DSDD side 2
note side 2 works now
DENSITY MFM,LOW CYLINDERS 82 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 193,194,195,196,197,198,199,200,201,202
SIDE2 0 193,194,195,196,197,198,199,200,201,202
note SIDE2 0 193,198,194,199,195,200,196,201,197,202
ORDER eagle
BSH 004h BLM 00fh EXM 001h DSM 0cch DRM 03fh AL0 080h AL1 000h OFS 82
END

BEGIN &BIG  Amstrad ReadBIG
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 41H,42H,43H,44H,45H,46H,47H,48H,49H
SIDE2 1 41H,42H,43H,44H,45H,46H,47H,48H,49H
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 355  DRM 127  AL0 0C0H  AL1 0  OFS 2
END

BEGIN &D10  Amstrad RAMDOS D10
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 11H,12H,13H,14H,15H,16H,17H,18H,19H,1AH
SIDE2 1 11H,12H,13H,14H,15H,16H,17H,18H,19H,1AH
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 400  DRM 127  AL0 0C0H  AL1 0  OFS 0
END

BEGIN &D20  Amstrad RAMDOS D20
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 31H,32H,33H,34H,35H,36H,37H,38H,39H,3AH
SIDE2 1 31H,32H,33H,34H,35H,36H,37H,38H,39H,3AH
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 400  DRM 255  AL0 0F0H  AL1 0  OFS 0
END

BEGIN CPC2  Amstrad CPC 'D20' - DSDD 96 tpi 3.50"
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512
SIDE1 0 031H,032H,033H,034H,035H,036H,037H,038H,039H,03AH
SIDE2 1 031H,032H,033H,034H,035H,036H,037H,038H,039H,03AH
ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 399 DRM 255 AL0 0F0H AL1 0 OFS 0
END

note BEGIN HD1  Hd-TestFormat 3.5"
note DENSITY MFM,HIGH CYLINDERS 80 SIDES 2 SECTORS 18,512
note SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note ORDER SIDES
note BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 0
note END

BEGIN D1   Romdos 716k Data (5.25")
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 01h, 02h, 03h, 04h, 05h, 06h, 07h, 08h, 09h
SIDE2 1 01h, 02h, 03h, 04h, 05h, 06h, 07h, 08h, 09h
ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 359 DRM 127 AL0 0c0H AL1 0 OFS 0
END

NOTE End of cpmdisks.def
